Static Call Graph - [.\build\Music Shield.axf]

# Static Call Graph for image .\build\Music Shield.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Mon Jul 27 18:17:33 2015

### Maximum Stack Usage = 1584 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ $Super$$main ⇒ Player::recordFile(char*) ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SVC_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SysTick_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - VolumeFlip() from main.o(.text) referenced 2 times from main.o(.text)
  - __default_new_handler() from arm_newhandler_noexceptions.o(.text) referenced from new.o(i._Znwj)
  - __default_terminate_handler() from arm_exceptions_globs.o(.text) referenced from arm_exceptions_globs.o(.text)
  - LEDflip() from main.o(.text) referenced from main.o(.text)
  - Pre_Next() from main.o(.text) referenced 2 times from main.o(.text)
  - fallFlip() from main.o(.text) referenced from main.o(.text)
  - riseFlip() from main.o(.text) referenced from main.o(.text)
  - FATDirHandle::readdir() from fatdirhandle.o(.text) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::seekdir(long) from fatdirhandle.o(.text) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::telldir() from fatdirhandle.o(.text) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::closedir() from fatdirhandle.o(.text) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::rewinddir() from fatdirhandle.o(.text) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::~FATDirHandle__deallocating() from fatdirhandle.o(i._ZN12FATDirHandleD0Ev) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - FATDirHandle::~FATDirHandle() from fatdirhandle.o(i._ZN12FATDirHandleD1Ev) referenced from fatdirhandle.o(.constdata__ZTV12FATDirHandle)
  - SDFileSystem::disk_write(const unsigned char*, unsigned long long) from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::disk_status() from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::disk_sectors() from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::disk_initialize() from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::disk_read(unsigned char*, unsigned long long) from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::disk_sync() from sdfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::~SDFileSystem() from player.o(i._ZN12SDFileSystemD1Ev) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - SDFileSystem::~SDFileSystem() from player.o(i._ZN12SDFileSystemD1Ev) referenced from player.o(.text)
  - FATFileHandle::flen() from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::read(void*, unsigned) from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::close() from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::fsync() from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::lseek(long, int) from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::write(const void*, unsigned) from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::isatty() from fatfilehandle.o(.text) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::~FATFileHandle__deallocating() from fatfilehandle.o(i._ZN13FATFileHandleD0Ev) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileHandle::~FATFileHandle() from fatfilehandle.o(i._ZN13FATFileHandleD1Ev) referenced from fatfilehandle.o(.constdata__ZTV13FATFileHandle)
  - FATFileSystem::disk_status() from fatfilesystem.o(i._ZN13FATFileSystem11disk_statusEv) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::disk_initialize() from fatfilesystem.o(i._ZN13FATFileSystem15disk_initializeEv) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::open(const char*, int) from fatfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - FATFileSystem::open(const char*, int) from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::mkdir(const char*, int) from fatfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - FATFileSystem::mkdir(const char*, int) from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::format() from fatfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - FATFileSystem::format() from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::remove(const char*) from fatfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - FATFileSystem::remove(const char*) from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::opendir(const char*) from fatfilesystem.o(.text) referenced from sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - FATFileSystem::opendir(const char*) from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::disk_sync() from fatfilesystem.o(i._ZN13FATFileSystem9disk_syncEv) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::~FATFileSystem__deallocating() from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - FATFileSystem::~FATFileSystem__sub_object() from fatfilesystem.o(.text) referenced from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - mbed::FileHandle::~FileHandle__sub_object() from retarget.o(i._ZN4mbed10FileHandleD2Ev) referenced from retarget.o(.constdata__ZTVN4mbed10FileHandleE)
  - mbed::TimerEvent::irq(unsigned) from TimerEvent.o(i._ZN4mbed10TimerEvent3irqEj) referenced from TimerEvent.o(i._ZN4mbed10TimerEventC2Ev)
  - mbed::TimerEvent::~TimerEvent__sub_object() from TimerEvent.o(i._ZN4mbed10TimerEventD2Ev) referenced from TimerEvent.o(.constdata__ZTVN4mbed10TimerEventE)
  - mbed::InterruptIn::_irq_handler(unsigned, gpio_irq_event) from InterruptIn.o(i._ZN4mbed11InterruptIn12_irq_handlerEj14gpio_irq_event) referenced from InterruptIn.o(i._ZN4mbed11InterruptInC1E7PinName)
  - mbed::InterruptIn::~InterruptIn() from InterruptIn.o(i._ZN4mbed11InterruptInD1Ev) referenced from InterruptIn.o(.constdata__ZTVN4mbed11InterruptInE)
  - mbed::InterruptIn::~InterruptIn() from InterruptIn.o(i._ZN4mbed11InterruptInD1Ev) referenced from main.o(.text)
  - mbed::BaseDirHandle::readdir() from FileSystemLike.o(i._ZN4mbed13BaseDirHandle7readdirEv) referenced from FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)
  - mbed::BaseDirHandle::closedir() from FileSystemLike.o(i._ZN4mbed13BaseDirHandle8closedirEv) referenced from FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)
  - mbed::BaseDirHandle::~BaseDirHandle__deallocating() from FileSystemLike.o(i._ZN4mbed13BaseDirHandleD0Ev) referenced from FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)
  - mbed::FileSystemLike::opendir(const char*) from FileSystemLike.o(i._ZN4mbed14FileSystemLike7opendirEPKc) referenced from FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)
  - mbed::FileSystemLike::~FileSystemLike__sub_object() from FileSystemLike.o(i._ZN4mbed14FileSystemLikeD2Ev) referenced from FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)
  - mbed::SPI::write(int) from SPI.o(i._ZN4mbed3SPI5writeEi) referenced from SPI.o(.constdata__ZTVN4mbed3SPIE)
  - mbed::Ticker::handler() from Ticker.o(i._ZN4mbed6Ticker7handlerEv) referenced from Ticker.o(.constdata__ZTVN4mbed6TickerE)
  - mbed::Ticker::~Ticker() from Ticker.o(i._ZN4mbed6TickerD1Ev) referenced from Ticker.o(.constdata__ZTVN4mbed6TickerE)
  - mbed::Ticker::~Ticker() from Ticker.o(i._ZN4mbed6TickerD1Ev) referenced from main.o(.text)
  - mbed::FileBase::~FileBase() from FileBase.o(i._ZN4mbed8FileBaseD1Ev) referenced from FileBase.o(.constdata__ZTVN4mbed8FileBaseE)
  - vs10xx::~vs10xx() from player.o(i._ZN6vs10xxD1Ev) referenced from player.o(.text)
  - __cxa_pure_virtual from pure_virt.o(i.__cxa_pure_virtual) referenced 3 times from fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - __cxa_pure_virtual from pure_virt.o(i.__cxa_pure_virtual) referenced 6 times from retarget.o(.constdata__ZTVN4mbed10FileHandleE)
  - __cxa_pure_virtual from pure_virt.o(i.__cxa_pure_virtual) referenced from TimerEvent.o(.constdata__ZTVN4mbed10TimerEventE)
  - __cxa_pure_virtual from pure_virt.o(i.__cxa_pure_virtual) referenced from FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)
  - __cxa_pure_virtual from pure_virt.o(i.__cxa_pure_virtual) referenced 3 times from fatdirhandle.o(.constdata__ZTVN4mbed9DirHandleE)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - __sti___10_player_cpp from player.o(.text) referenced from player.o(.init_array)
  - __sti___8_main_cpp from main.o(.text) referenced from main.o(.init_array)
  - _sbackspace from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0fprintf)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0printf)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0vfprintf)
  - gpio_irq0 from gpio_irq_api.o(i.gpio_irq0) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq1 from gpio_irq_api.o(i.gpio_irq1) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq2 from gpio_irq_api.o(i.gpio_irq2) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq3 from gpio_irq_api.o(i.gpio_irq3) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq4 from gpio_irq_api.o(i.gpio_irq4) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq5 from gpio_irq_api.o(i.gpio_irq5) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - gpio_irq6 from gpio_irq_api.o(i.gpio_irq6) referenced from gpio_irq_api.o(i.gpio_irq_init)
  - isspace from isspace_c.o(.text) referenced from scanf_char.o(.text)
  - main from retarget.o(i.$Sub$$main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - rtc_init from rtc_api.o(i.rtc_init) referenced from rtc_time.o(.data)
  - rtc_isenabled from rtc_api.o(i.rtc_isenabled) referenced from rtc_time.o(.data)
  - rtc_read from rtc_api.o(i.rtc_read) referenced from rtc_time.o(.data)
  - rtc_write from rtc_api.o(i.rtc_write) referenced from rtc_time.o(.data)
  - timer_irq_handler from hal_tick.o(i.timer_irq_handler) referenced from hal_tick.o(i.HAL_InitTick)
  - us_ticker_clear_interrupt from us_ticker.o(i.us_ticker_clear_interrupt) referenced from us_ticker_api.o(.constdata)
  - us_ticker_disable_interrupt from us_ticker.o(i.us_ticker_disable_interrupt) referenced from us_ticker_api.o(.constdata)
  - us_ticker_init from us_ticker.o(i.us_ticker_init) referenced from us_ticker_api.o(.constdata)
  - us_ticker_read from us_ticker.o(i.us_ticker_read) referenced from us_ticker_api.o(.constdata)
  - us_ticker_set_interrupt from us_ticker.o(i.us_ticker_set_interrupt) referenced from us_ticker_api.o(.constdata)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  __use_full_stdio (Thumb, 0 bytes, Stack size unknown bytes, entry6b.o(.ARM.Collect$$$$00000006))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = __use_full_stdio ⇒ _initio ⇒ _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _initio

  __main_after_initio (Thumb, 0 bytes, Stack size unknown bytes, entry6b.o(.ARM.Collect$$$$00000006))
  [Called By]

  - >> _initio

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init$empty (Thumb, 0 bytes, Stack size unknown bytes, entry8a.o(.ARM.Collect$$$$00000009))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = _main_cpp_init$empty ⇒ __cpp_initialize__aeabi_
  [Calls]
  - >> __cpp_initialize__aeabi_

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  LEDflip() (Thumb, 112 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = LEDflip() ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed_assert_internal
  [Address Reference Count : 1]
  - main.o(.text)

  fallFlip() (Thumb, 14 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fallFlip() ⇒ mbed::Timer::read_ms()
  [Calls]
  - >> mbed::Timer::read_ms()
  [Address Reference Count : 1]
  - main.o(.text)

  riseFlip() (Thumb, 52 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = riseFlip() ⇒ mbed::Timer::read_ms()
  [Calls]
  - >> mbed::Timer::read_ms()
  [Address Reference Count : 1]
  - main.o(.text)

  VolumeFlip() (Thumb, 98 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = VolumeFlip() ⇒ mbed::InterruptIn::operator int() ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::InterruptIn::operator int()
  - >> __2printf
  [Address Reference Count : 1]
  - main.o(.text)

  Pre_Next() (Thumb, 78 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = Pre_Next() ⇒ mbed::InterruptIn::operator int() ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::InterruptIn::operator int()
  [Address Reference Count : 1]
  - main.o(.text)

  $Super$$main (Thumb, 168 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 1576
  - Call Chain = $Super$$main ⇒ Player::recordFile(char*) ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> mbed::FunctionPointerArg1⟨void, void⟩::attach(void(*)())
  - >> __aeabi_fmul
  - >> __aeabi_f2uiz
  - >> Player::playFile(char*)
  - >> Player::begin()
  - >> Player::recordFile(char*)
  - >> mbed::Ticker::setup(unsigned)
  - >> mbed::Timer::start()
  - >> mbed::InterruptIn::rise(void(*)())
  - >> mbed::InterruptIn::fall(void(*)())
  [Called By]
  - >> main

  vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) (Thumb, 142 bytes, Stack size 40 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalOut::DigitalOut(PinName)
  - >> gpio_init_in
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::DigitalOut::operator =(int)
  - >> __aeabi_memclr4
  [Called By]
  - >> __sti___10_player_cpp

  vs10xx::vs10xx__sub_object(PinName, PinName, PinName, PinName, PinName, PinName, PinName) (Thumb, 0 bytes, Stack size 40 bytes, vs10xx.o(.text), UNUSED)

  vs10xx::writeRegister(unsigned char, unsigned) (Thumb, 86 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> vs10xx::loadPlugin(const unsigned short*, int)
  - >> vs10xx::setVolume(unsigned char)
  - >> vs10xx::softReset()
  - >> Player::playFile(char*)
  - >> Player::recordFile(char*)

  vs10xx::readRegister(unsigned char) (Thumb, 92 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = vs10xx::readRegister(unsigned char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> vs10xx::softReset()
  - >> Player::recordFile(char*)

  vs10xx::writeData(unsigned char*, unsigned char) (Thumb, 76 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = vs10xx::writeData(unsigned char*, unsigned char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> Player::playFile(char*)

  vs10xx::softReset() (Thumb, 168 bytes, Stack size 8 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = vs10xx::softReset() ⇒ vs10xx::readRegister(unsigned char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> wait_ms
  - >> mbed::SPI::frequency(int)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> __2printf
  [Called By]
  - >> vs10xx::reset()
  - >> Player::playFile(char*)
  - >> Player::recordFile(char*)

  vs10xx::reset() (Thumb, 66 bytes, Stack size 8 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = vs10xx::reset() ⇒ vs10xx::softReset() ⇒ vs10xx::readRegister(unsigned char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> wait_ms
  - >> mbed::SPI::write(int)
  - >> vs10xx::softReset()
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> Player::begin()

  vs10xx::setFreq(int) (Thumb, 16 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = vs10xx::setFreq(int) ⇒ mbed::SPI::frequency(int) ⇒ spi_frequency ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> mbed::SPI::frequency(int)
  [Called By]
  - >> Player::playFile(char*)

  vs10xx::setVolume(unsigned char) (Thumb, 20 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> vs10xx::writeRegister(unsigned char, unsigned)

  vs10xx::loadPlugin(const unsigned short*, int) (Thumb, 116 bytes, Stack size 32 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  [Called By]
  - >> Player::playFile(char*)
  - >> Player::recordFile(char*)

  Set32(unsigned char*, unsigned) (Thumb, 18 bytes, Stack size 0 bytes, player.o(.text))
  [Called By]

  - >> Player::recordFile(char*)

  Player::begin() (Thumb, 282 bytes, Stack size 32 bytes, player.o(.text))
  [Stack]

  - Max Depth = 1568
  - Call Chain = Player::begin() ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> std::strstr(char*, const char*)
  - >> opendir
  - >> FATFileSystem::open(const char*, int)
  - >> vs10xx::reset()
  - >> __2printf
  [Called By]
  - >> $Super$$main

  Player::playFile(char*) (Thumb, 284 bytes, Stack size 24 bytes, player.o(.text))
  [Stack]

  - Max Depth = 1560
  - Call Chain = Player::playFile(char*) ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> std::strstr(char*, const char*)
  - >> FATFileSystem::open(const char*, int)
  - >> vs10xx::loadPlugin(const unsigned short*, int)
  - >> vs10xx::setFreq(int)
  - >> vs10xx::softReset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> __2printf
  [Called By]
  - >> $Super$$main

  Player::recordFile(char*) (Thumb, 302 bytes, Stack size 40 bytes, player.o(.text))
  [Stack]

  - Max Depth = 1576
  - Call Chain = Player::recordFile(char*) ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> FATFileSystem::remove(const char*)
  - >> FATFileSystem::open(const char*, int)
  - >> Set32(unsigned char*, unsigned)
  - >> vs10xx::loadPlugin(const unsigned short*, int)
  - >> vs10xx::softReset()
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> __2printf
  [Called By]
  - >> $Super$$main

  SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*) (Thumb, 96 bytes, Stack size 40 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::DigitalOut::operator =(int)
  - >> gpio_init_out
  - >> FATFileSystem::FATFileSystem__sub_object(const char*)
  - >> __aeabi_memclr4
  [Called By]
  - >> __sti___10_player_cpp

  SDFileSystem::SDFileSystem__sub_object(PinName, PinName, PinName, PinName, const char*) (Thumb, 0 bytes, Stack size 40 bytes, sdfilesystem.o(.text), UNUSED)

  SDFileSystem::_cmd(int, int) (Thumb, 166 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_cmd(int, int) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::disk_write(const unsigned char*, unsigned long long)
  - >> SDFileSystem::disk_read(unsigned char*, unsigned long long)
  - >> SDFileSystem::disk_initialize()
  - >> SDFileSystem::initialise_card()
  - >> SDFileSystem::initialise_card_v2()
  - >> SDFileSystem::initialise_card_v1()

  SDFileSystem::_read(unsigned char*, unsigned) (Thumb, 104 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_read(unsigned char*, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::disk_read(unsigned char*, unsigned long long)
  - >> SDFileSystem::_sd_sectors()

  SDFileSystem::_cmdx(int, int) (Thumb, 146 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_cmdx(int, int) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::_sd_sectors()

  SDFileSystem::_sd_sectors() (Thumb, 270 bytes, Stack size 88 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = SDFileSystem::_sd_sectors() ⇒ SDFileSystem::_cmdx(int, int) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> debug(const char*, ...)
  - >> ext_bits(unsigned char*, int, int)
  - >> debug_if(int, const char*, ...)
  - >> SDFileSystem::_cmdx(int, int)
  - >> SDFileSystem::_read(unsigned char*, unsigned)
  [Called By]
  - >> SDFileSystem::disk_initialize()

  SDFileSystem::initialise_card_v1() (Thumb, 70 bytes, Stack size 16 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = SDFileSystem::initialise_card_v1() ⇒ SDFileSystem::_cmd(int, int) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> debug(const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> SDFileSystem::_cmd(int, int)
  [Called By]
  - >> SDFileSystem::initialise_card()

  SDFileSystem::_cmd58() (Thumb, 506 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_cmd58() ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::initialise_card_v2()

  SDFileSystem::initialise_card_v2() (Thumb, 88 bytes, Stack size 16 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = SDFileSystem::initialise_card_v2() ⇒ SDFileSystem::_cmd58() ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> debug(const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> wait_ms
  - >> SDFileSystem::_cmd58()
  - >> SDFileSystem::_cmd(int, int)
  [Called By]
  - >> SDFileSystem::initialise_card()

  SDFileSystem::_cmd8() (Thumb, 190 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_cmd8() ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::initialise_card()

  SDFileSystem::initialise_card() (Thumb, 110 bytes, Stack size 16 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = SDFileSystem::initialise_card() ⇒ SDFileSystem::initialise_card_v2() ⇒ SDFileSystem::_cmd58() ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> debug(const char*, ...)
  - >> mbed::SPI::frequency(int)
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  - >> SDFileSystem::_cmd8()
  - >> SDFileSystem::initialise_card_v2()
  - >> SDFileSystem::initialise_card_v1()
  - >> SDFileSystem::_cmd(int, int)
  [Called By]
  - >> SDFileSystem::disk_initialize()

  SDFileSystem::disk_initialize() (Thumb, 72 bytes, Stack size 16 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 240
  - Call Chain = SDFileSystem::disk_initialize() ⇒ SDFileSystem::_sd_sectors() ⇒ SDFileSystem::_cmdx(int, int) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> debug(const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> mbed::SPI::frequency(int)
  - >> SDFileSystem::initialise_card()
  - >> SDFileSystem::_sd_sectors()
  - >> SDFileSystem::_cmd(int, int)
  [Address Reference Count : 1]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  SDFileSystem::disk_status() (Thumb, 6 bytes, Stack size 0 bytes, sdfilesystem.o(.text))
  [Address Reference Count : 1]

  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  SDFileSystem::disk_read(unsigned char*, unsigned long long) (Thumb, 54 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = SDFileSystem::disk_read(unsigned char*, unsigned long long) ⇒ SDFileSystem::_read(unsigned char*, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SDFileSystem::_read(unsigned char*, unsigned)
  - >> SDFileSystem::_cmd(int, int)
  [Address Reference Count : 1]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  SDFileSystem::_write(const unsigned char*, unsigned) (Thumb, 154 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = SDFileSystem::_write(const unsigned char*, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::SPI::write(int)
  - >> mbed::DigitalOut::operator =(int)
  [Called By]
  - >> SDFileSystem::disk_write(const unsigned char*, unsigned long long)

  SDFileSystem::disk_write(const unsigned char*, unsigned long long) (Thumb, 54 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = SDFileSystem::disk_write(const unsigned char*, unsigned long long) ⇒ SDFileSystem::_write(const unsigned char*, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SDFileSystem::_write(const unsigned char*, unsigned)
  - >> SDFileSystem::_cmd(int, int)
  [Address Reference Count : 1]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  SDFileSystem::disk_sync() (Thumb, 6 bytes, Stack size 0 bytes, sdfilesystem.o(.text))
  [Address Reference Count : 1]

  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  SDFileSystem::disk_sectors() (Thumb, 10 bytes, Stack size 0 bytes, sdfilesystem.o(.text))
  [Address Reference Count : 1]

  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)

  FATDirHandle::FATDirHandle(const FATFS_DIR&) (Thumb, 26 bytes, Stack size 16 bytes, fatdirhandle.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = FATDirHandle::FATDirHandle(const FATFS_DIR&) ⇒ __aeabi_memcpy4
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> FATFileSystem::opendir(const char*)

  FATDirHandle::FATDirHandle__sub_object(const FATFS_DIR&) (Thumb, 0 bytes, Stack size 16 bytes, fatdirhandle.o(.text), UNUSED)

  FATDirHandle::closedir() (Thumb, 18 bytes, Stack size 8 bytes, fatdirhandle.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = FATDirHandle::closedir()
  [Address Reference Count : 1]
  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::readdir() (Thumb, 68 bytes, Stack size 48 bytes, fatdirhandle.o(.text))
  [Stack]

  - Max Depth = 296
  - Call Chain = FATDirHandle::readdir() ⇒ f_readdir ⇒ dir_read(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_readdir
  - >> __aeabi_memcpy
  [Address Reference Count : 1]
  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::rewinddir() (Thumb, 6 bytes, Stack size 0 bytes, fatdirhandle.o(.text))
  [Address Reference Count : 1]

  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::telldir() (Thumb, 6 bytes, Stack size 0 bytes, fatdirhandle.o(.text))
  [Address Reference Count : 1]

  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::seekdir(long) (Thumb, 4 bytes, Stack size 0 bytes, fatdirhandle.o(.text))
  [Address Reference Count : 1]

  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATFileHandle::FATFileHandle(FIL) (Thumb, 32 bytes, Stack size 24 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = FATFileHandle::FATFileHandle(FIL) ⇒ __aeabi_memcpy4
  [Calls]
  - >> __aeabi_memcpy4
  [Called By]
  - >> FATFileSystem::open(const char*, int)

  FATFileHandle::FATFileHandle__sub_object(FIL) (Thumb, 0 bytes, Stack size 24 bytes, fatfilehandle.o(.text), UNUSED)

  FATFileHandle::close() (Thumb, 26 bytes, Stack size 16 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = FATFileHandle::close() ⇒ f_close ⇒ f_sync ⇒ sync(FATFS*) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_close
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::write(const void*, unsigned) (Thumb, 44 bytes, Stack size 24 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 248
  - Call Chain = FATFileHandle::write(const void*, unsigned) ⇒ f_write ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_write
  - >> debug_if(int, const char*, ...)
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::read(void*, unsigned) (Thumb, 54 bytes, Stack size 24 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 208
  - Call Chain = FATFileHandle::read(void*, unsigned) ⇒ f_read ⇒ get_fat(FATFS*, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_read
  - >> debug_if(int, const char*, ...)
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::isatty() (Thumb, 6 bytes, Stack size 0 bytes, fatfilehandle.o(.text))
  [Address Reference Count : 1]

  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::lseek(long, int) (Thumb, 72 bytes, Stack size 24 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = FATFileHandle::lseek(long, int) ⇒ f_lseek ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_lseek
  - >> debug_if(int, const char*, ...)
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::fsync() (Thumb, 34 bytes, Stack size 16 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = FATFileHandle::fsync() ⇒ f_sync ⇒ sync(FATFS*) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_sync
  - >> debug_if(int, const char*, ...)
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::flen() (Thumb, 6 bytes, Stack size 0 bytes, fatfilehandle.o(.text))
  [Address Reference Count : 1]

  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  get_fattime (Thumb, 60 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = get_fattime ⇒ time
  [Calls]
  - >> time
  - >> localtime
  [Called By]
  - >> f_open
  - >> f_mkfs
  - >> f_mkdir
  - >> f_sync

  FATFileSystem::FATFileSystem__sub_object(const char*) (Thumb, 98 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = FATFileSystem::FATFileSystem__sub_object(const char*) ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> f_mount
  - >> error
  - >> mbed::FileSystemLike::FileSystemLike__sub_object(const char*)
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)

  FATFileSystem::~FATFileSystem() (Thumb, 0 bytes, Stack size 16 bytes, fatfilesystem.o(.text), UNUSED)

  FATFileSystem::~FATFileSystem__sub_object() (Thumb, 56 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = FATFileSystem::~FATFileSystem__sub_object()
  [Calls]
  - >> f_mount
  - >> mbed::FileSystemLike::~FileSystemLike__sub_object()
  [Called By]
  - >> SDFileSystem::~SDFileSystem()
  - >> FATFileSystem::~FATFileSystem__deallocating()
  [Address Reference Count : 1]
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::~FATFileSystem__deallocating() (Thumb, 18 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = FATFileSystem::~FATFileSystem__deallocating() ⇒ FATFileSystem::~FATFileSystem__sub_object()
  [Calls]
  - >> FATFileSystem::~FATFileSystem__sub_object()
  - >> operator delete (void*)
  [Address Reference Count : 1]
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::open(const char*, int) (Thumb, 178 bytes, Stack size 1176 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 1536
  - Call Chain = FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_open
  - >> debug_if(int, const char*, ...)
  - >> f_lseek
  - >> FATFileHandle::FATFileHandle(FIL)
  - >> operator new(unsigned)
  - >> __2sprintf
  - >> __aeabi_memcpy4
  [Called By]
  - >> Player::playFile(char*)
  - >> Player::begin()
  - >> Player::recordFile(char*)
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::remove(const char*) (Thumb, 36 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 368
  - Call Chain = FATFileSystem::remove(const char*) ⇒ f_unlink ⇒ follow_path(FATFS_DIR*, const char*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_unlink
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> Player::recordFile(char*)
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::format() (Thumb, 42 bytes, Stack size 16 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = FATFileSystem::format() ⇒ f_mkfs ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_mkfs
  - >> debug_if(int, const char*, ...)
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::opendir(const char*) (Thumb, 46 bytes, Stack size 56 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 344
  - Call Chain = FATFileSystem::opendir(const char*) ⇒ f_opendir ⇒ follow_path(FATFS_DIR*, const char*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_opendir
  - >> FATDirHandle::FATDirHandle(const FATFS_DIR&)
  - >> operator new(unsigned)
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::mkdir(const char*, int) (Thumb, 32 bytes, Stack size 24 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 384
  - Call Chain = FATFileSystem::mkdir(const char*, int) ⇒ f_mkdir ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_mkdir
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  ff_convert (Thumb, 70 bytes, Stack size 8 bytes, ccsbcs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ff_convert
  [Called By]
  - >> get_fileinfo(FATFS_DIR*, FILINFO*)
  - >> create_name(FATFS_DIR*, const char**)

  ff_wtoupper (Thumb, 46 bytes, Stack size 0 bytes, ccsbcs.o(.text))
  [Called By]

  - >> cmp_lfn(unsigned short*, unsigned char*)

  disk_initialize(unsigned char) (Thumb, 34 bytes, Stack size 8 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = disk_initialize(unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> f_mkfs

  disk_status(unsigned char) (Thumb, 34 bytes, Stack size 8 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = disk_status(unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> validate(void*)
  - >> chk_mounted(const char**, FATFS**, unsigned char)

  disk_read(unsigned char, unsigned char*, unsigned long, unsigned char) (Thumb, 96 bytes, Stack size 32 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = disk_read(unsigned char, unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> check_fs(FATFS*, unsigned long)
  - >> move_window(FATFS*, unsigned long)
  - >> f_write
  - >> f_read
  - >> f_lseek

  disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) (Thumb, 96 bytes, Stack size 32 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> sync(FATFS*)
  - >> move_window(FATFS*, unsigned long)
  - >> f_mkfs
  - >> f_write
  - >> f_sync
  - >> f_read
  - >> f_lseek

  disk_ioctl(unsigned char, unsigned char, void*) (Thumb, 126 bytes, Stack size 24 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = disk_ioctl(unsigned char, unsigned char, void*) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> debug_if(int, const char*, ...)
  [Called By]
  - >> sync(FATFS*)
  - >> f_mkfs

  clust2sect(FATFS*, unsigned long) (Thumb, 26 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_rename
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> f_mkdir
  - >> f_write
  - >> f_read
  - >> f_lseek

  get_fat(FATFS*, unsigned long) (Thumb, 228 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = get_fat(FATFS*, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> move_window(FATFS*, unsigned long)
  [Called By]
  - >> f_truncate
  - >> f_getfree
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> create_chain(FATFS*, unsigned long)
  - >> remove_chain(FATFS*, unsigned long)
  - >> f_read
  - >> f_lseek

  put_fat(FATFS*, unsigned long, unsigned long) (Thumb, 314 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> move_window(FATFS*, unsigned long)
  [Called By]
  - >> f_truncate
  - >> create_chain(FATFS*, unsigned long)
  - >> remove_chain(FATFS*, unsigned long)

  gen_numname(unsigned char*, const unsigned char*, const unsigned short*, unsigned short) (Thumb, 168 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = gen_numname(unsigned char*, const unsigned char*, const unsigned short*, unsigned short) ⇒ mem_cpy(void*, const void*, unsigned)
  [Calls]
  - >> mem_cpy(void*, const void*, unsigned)
  [Called By]
  - >> dir_register(FATFS_DIR*)

  f_mount (Thumb, 38 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> FATFileSystem::~FATFileSystem__sub_object()
  - >> FATFileSystem::FATFileSystem__sub_object(const char*)

  f_open (Thumb, 370 bytes, Stack size 88 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 360
  - Call Chain = f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_register(FATFS_DIR*)
  - >> st_clust(unsigned char*, unsigned long)
  - >> ld_clust(FATFS*, unsigned char*)
  - >> remove_chain(FATFS*, unsigned long)
  - >> move_window(FATFS*, unsigned long)
  - >> get_fattime
  [Called By]
  - >> FATFileSystem::open(const char*, int)

  f_read (Thumb, 458 bytes, Stack size 64 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 184
  - Call Chain = f_read ⇒ get_fat(FATFS*, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> get_fat(FATFS*, unsigned long)
  - >> clust2sect(FATFS*, unsigned long)
  - >> validate(void*)
  - >> mem_cpy(void*, const void*, unsigned)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> FATFileHandle::read(void*, unsigned)

  f_write (Thumb, 522 bytes, Stack size 64 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 224
  - Call Chain = f_write ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> clust2sect(FATFS*, unsigned long)
  - >> validate(void*)
  - >> create_chain(FATFS*, unsigned long)
  - >> mem_cpy(void*, const void*, unsigned)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> FATFileHandle::write(const void*, unsigned)

  f_sync (Thumb, 174 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = f_sync ⇒ sync(FATFS*) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> validate(void*)
  - >> st_clust(unsigned char*, unsigned long)
  - >> sync(FATFS*)
  - >> move_window(FATFS*, unsigned long)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> get_fattime
  [Called By]
  - >> f_close
  - >> FATFileHandle::fsync()

  f_close (Thumb, 22 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = f_close ⇒ f_sync ⇒ sync(FATFS*) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> f_sync
  [Called By]
  - >> FATFileHandle::close()

  f_lseek (Thumb, 430 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = f_lseek ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> get_fat(FATFS*, unsigned long)
  - >> clust2sect(FATFS*, unsigned long)
  - >> validate(void*)
  - >> create_chain(FATFS*, unsigned long)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> FATFileSystem::open(const char*, int)
  - >> FATFileHandle::lseek(long, int)

  f_opendir (Thumb, 116 bytes, Stack size 40 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 288
  - Call Chain = f_opendir ⇒ follow_path(FATFS_DIR*, const char*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> ld_clust(FATFS*, unsigned char*)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  [Called By]
  - >> FATFileSystem::opendir(const char*)

  f_readdir (Thumb, 90 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 248
  - Call Chain = f_readdir ⇒ dir_read(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> validate(void*)
  - >> get_fileinfo(FATFS_DIR*, FILINFO*)
  - >> dir_read(FATFS_DIR*)
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  [Called By]
  - >> FATDirHandle::readdir()

  f_stat (Thumb, 62 bytes, Stack size 72 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> get_fileinfo(FATFS_DIR*, FILINFO*)

  f_getfree (Thumb, 260 bytes, Stack size 56 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> get_fat(FATFS*, unsigned long)
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> move_window(FATFS*, unsigned long)

  f_truncate (Thumb, 160 bytes, Stack size 16 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> put_fat(FATFS*, unsigned long, unsigned long)
  - >> get_fat(FATFS*, unsigned long)
  - >> validate(void*)
  - >> remove_chain(FATFS*, unsigned long)

  f_unlink (Thumb, 172 bytes, Stack size 104 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 352
  - Call Chain = f_unlink ⇒ follow_path(FATFS_DIR*, const char*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_remove(FATFS_DIR*)
  - >> dir_read(FATFS_DIR*)
  - >> ld_clust(FATFS*, unsigned char*)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> remove_chain(FATFS*, unsigned long)
  - >> sync(FATFS*)
  - >> mem_cpy(void*, const void*, unsigned)
  [Called By]
  - >> FATFileSystem::remove(const char*)

  f_mkdir (Thumb, 364 bytes, Stack size 88 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 360
  - Call Chain = f_mkdir ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> clust2sect(FATFS*, unsigned long)
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_register(FATFS_DIR*)
  - >> st_clust(unsigned char*, unsigned long)
  - >> create_chain(FATFS*, unsigned long)
  - >> remove_chain(FATFS*, unsigned long)
  - >> sync(FATFS*)
  - >> move_window(FATFS*, unsigned long)
  - >> mem_set(void*, int, unsigned)
  - >> mem_cpy(void*, const void*, unsigned)
  - >> get_fattime
  [Called By]
  - >> FATFileSystem::mkdir(const char*, int)

  f_chmod (Thumb, 88 bytes, Stack size 80 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> sync(FATFS*)

  f_utime (Thumb, 90 bytes, Stack size 72 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> sync(FATFS*)

  f_rename (Thumb, 280 bytes, Stack size 144 bytes, ff.o(.text), UNUSED)
  [Calls]

  - >> clust2sect(FATFS*, unsigned long)
  - >> chk_mounted(const char**, FATFS**, unsigned char)
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_remove(FATFS_DIR*)
  - >> dir_register(FATFS_DIR*)
  - >> st_clust(unsigned char*, unsigned long)
  - >> ld_clust(FATFS*, unsigned char*)
  - >> sync(FATFS*)
  - >> move_window(FATFS*, unsigned long)
  - >> mem_cpy(void*, const void*, unsigned)

  f_mkfs (Thumb, 1536 bytes, Stack size 104 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = f_mkfs ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> mem_set(void*, int, unsigned)
  - >> mem_cpy(void*, const void*, unsigned)
  - >> disk_ioctl(unsigned char, unsigned char, void*)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_initialize(unsigned char)
  - >> get_fattime
  [Called By]
  - >> FATFileSystem::format()

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  _initio (Thumb, 20 bytes, Stack size 0 bytes, initio_oe.o(.text))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = _initio ⇒ _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _sys_open
  - >> __main_after_initio
  [Called By]
  - >> __use_full_stdio

  fflush (Thumb, 38 bytes, Stack size 16 bytes, fflush_fe.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fflush
  [Calls]
  - >> _sys_seek
  - >> _sys_ensure
  [Called By]
  - >> exit

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod
  - >> __aeabi_d2ulz
  - >> _double_epilogue

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  mktime (Thumb, 142 bytes, Stack size 16 bytes, mktime.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = mktime ⇒ _localtime
  [Calls]
  - >> _localtime
  [Called By]
  - >> rtc_read

  ___aeabi_memcpy8$move (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 64 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy
  [Called By]
  - >> FATDirHandle::readdir()

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memcpy4
  [Called By]
  - >> FATFileSystem::open(const char*, int)
  - >> FATFileHandle::FATFileHandle(FIL)
  - >> FATDirHandle::FATDirHandle(const FATFS_DIR&)

  __aeabi_memmove (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memmove4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memmove4
  [Called By]
  - >> NVIC_SetVector

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)
  - >> mbed::DigitalOut::DigitalOut(PinName)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> __sti___8_main_cpp
  - >> mbed::FileSystemLike::opendir()

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> std::strstr(char*, const char*)

  strncpy (Thumb, 24 bytes, Stack size 8 bytes, strncpy.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strncpy
  [Called By]
  - >> mbed::BaseDirHandle::readdir()

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> mbed::FileBase::lookup(const char*, unsigned)

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> _sys_open

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> mbed::FileBase::lookup(const char*, unsigned)

  __0sscanf (Thumb, 48 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> _sys_open

  _scanf_int (Thumb, 336 bytes, Stack size 56 bytes, _scanf_int.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_int
  [Calls]
  - >> _chval
  [Called By]
  - >> __vfscanf

  __cpp_initialize__aeabi_ (Thumb, 22 bytes, Stack size 16 bytes, cpp_init.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __cpp_initialize__aeabi_
  [Called By]
  - >> _main_cpp_init$empty

  __aeabi_fmul (Thumb, 108 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> $Super$$main

  __aeabi_f2uiz (Thumb, 40 bytes, Stack size 0 bytes, ffixui.o(.text))
  [Called By]

  - >> $Super$$main

  __default_new_handler() (Thumb, 4 bytes, Stack size 0 bytes, arm_newhandler_noexceptions.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = __default_new_handler() ⇒ std::terminate() ⇒ __cxa_get_globals ⇒ __ARM_exceptions_buffer_init ⇒ malloc
  [Calls]
  - >> std::terminate()
  [Address Reference Count : 1]
  - new.o(i._Znwj)

  fputc (Thumb, 40 bytes, Stack size 16 bytes, fputc_fp.o(.text))
  [Stack]

  - Max Depth = 232
  - Call Chain = fputc ⇒ _sys_write ⇒ serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> _sys_write
  [Address Reference Count : 3]
  - printfa.o(i.__0fprintf)
  - printfa.o(i.__0printf)
  - printfa.o(i.__0vfprintf)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  localtime (Thumb, 6 bytes, Stack size 0 bytes, localtime_w.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = localtime ⇒ _localtime
  [Calls]
  - >> _localtime
  [Called By]
  - >> get_fattime
  - >> rtc_write

  _localtime (Thumb, 122 bytes, Stack size 12 bytes, localtime_i.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = _localtime
  [Called By]
  - >> localtime
  - >> mktime

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_int

  __vfscanf_char (Thumb, 20 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  __rt_ddtor_pointer_addr (Thumb, 4 bytes, Stack size 0 bytes, cpp_dtor.o(.text))
  [Called By]

  - >> __aeabi_atexit
  - >> __cxa_finalize

  __rt_lib_shutdown_cpp_1 (Thumb, 2 bytes, Stack size 0 bytes, cpp_final.o(.text), UNUSED)

  __rt_new_handler_addr (Thumb, 4 bytes, Stack size 0 bytes, cpp_memory.o(.text))
  [Called By]

  - >> operator new(unsigned)

  __rt_SIGPVFN (Thumb, 2 bytes, Stack size 0 bytes, cpp_signal.o(.text))
  [Called By]

  - >> __cxa_pure_virtual

  __aeabi_unwind_cpp_pr0 (Thumb, 4 bytes, Stack size 0 bytes, cpp_unwinder.o(.text), UNUSED)

  __aeabi_unwind_cpp_pr1 (Thumb, 4 bytes, Stack size 0 bytes, cpp_unwinder.o(.text), UNUSED)

  _Unwind_DeleteException (Thumb, 2 bytes, Stack size 0 bytes, cpp_unwinder.o(.text), UNUSED)

  _Unwind_Activity (Thumb, 2 bytes, Stack size 0 bytes, cpp_unwinder.o(.text), UNUSED)

  _Unwind_RaiseException (Thumb, 4 bytes, Stack size 0 bytes, cpp_unwinder.o(.text), UNUSED)

  __rt_eh_globals_addr (Thumb, 10 bytes, Stack size 0 bytes, cpp_unwinder.o(.text))
  [Called By]

  - >> __cxa_get_globals

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> _fp_digits
  - >> __aeabi_drsub
  - >> __aeabi_dsub

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 38 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  std::terminate() (Thumb, 26 bytes, Stack size 8 bytes, arm_exceptions_terminate.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = std::terminate() ⇒ __cxa_get_globals ⇒ __ARM_exceptions_buffer_init ⇒ malloc
  [Calls]
  - >> __cxa_get_globals
  [Called By]
  - >> __default_new_handler()

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  isspace (Thumb, 10 bytes, Stack size 0 bytes, isspace_c.o(.text))
  [Calls]

  - >> __ctype_lookup
  [Address Reference Count : 1]
  - scanf_char.o(.text)

  __vfscanf (Thumb, 806 bytes, Stack size 88 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _scanf_int
  [Called By]
  - >> __vfscanf_char

  _double_round (Thumb, 26 bytes, Stack size 8 bytes, depilogue.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _double_epilogue

  _double_epilogue (Thumb, 164 bytes, Stack size 32 bytes, depilogue.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __cxa_get_globals (Thumb, 62 bytes, Stack size 16 bytes, arm_exceptions_globs.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = __cxa_get_globals ⇒ __ARM_exceptions_buffer_init ⇒ malloc
  [Calls]
  - >> malloc
  - >> __ARM_exceptions_buffer_init
  - >> __rt_eh_globals_addr
  [Called By]
  - >> std::terminate()

  __ctype_lookup (Thumb, 34 bytes, Stack size 0 bytes, ctype_c.o(.text))
  [Called By]

  - >> isspace

  __ARM_exceptions_buffer_init (Thumb, 18 bytes, Stack size 8 bytes, arm_exceptions_mem.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = __ARM_exceptions_buffer_init ⇒ malloc
  [Calls]
  - >> malloc
  [Called By]
  - >> __cxa_get_globals

  __ARM_exceptions_buffer_allocate (Thumb, 22 bytes, Stack size 0 bytes, arm_exceptions_mem.o(.text), UNUSED)

  __ARM_exceptions_buffer_free (Thumb, 20 bytes, Stack size 0 bytes, arm_exceptions_mem.o(.text), UNUSED)

  main (Thumb, 18 bytes, Stack size 8 bytes, retarget.o(i.$Sub$$main))
  [Stack]

  - Max Depth = 1584
  - Call Chain = main ⇒ $Super$$main ⇒ Player::recordFile(char*) ⇒ FATFileSystem::open(const char*, int) ⇒ f_open ⇒ dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> $Super$$main
  - >> mbed_sdk_init
  - >> mbed_main
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCC_OscConfig

  HAL_GPIO_Init (Thumb, 454 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> pin_function

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RTC_Init
  - >> RTC_WriteTimeCounter
  - >> RTC_WriteAlarmCounter
  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> timer_irq_handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_MspInit
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  [Called By]
  - >> SystemInit
  - >> mbed_sdk_init

  HAL_InitTick (Thumb, 158 bytes, Stack size 16 bytes, hal_tick.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_TIM_OC_Start
  - >> HAL_TIM_Base_Start
  - >> HAL_TIM_Base_Init
  - >> SystemCoreClockUpdate
  - >> NVIC_SetVector
  [Called By]
  - >> HAL_Init
  - >> HAL_RCC_ClockConfig
  - >> us_ticker_set_interrupt
  - >> us_ticker_read
  - >> us_ticker_init

  HAL_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_MspInit))
  [Called By]

  - >> HAL_Init

  HAL_NVIC_SetPriorityGrouping (Thumb, 30 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_PWR_EnableBkUpAccess (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess))
  [Called By]

  - >> rtc_init

  HAL_RCCEx_GetPeriphCLKFreq (Thumb, 266 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_RCCEx_GetPeriphCLKFreq ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  [Called By]
  - >> HAL_RTC_Init

  HAL_RCC_ClockConfig (Thumb, 730 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SetSysClock

  HAL_RCC_GetPCLK1Freq (Thumb, 64 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 64 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCCEx_GetPeriphCLKFreq
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 124 bytes, Stack size 24 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_OscConfig (Thumb, 2306 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_Delay
  [Calls]
  - >> HAL_GetTick
  - >> HAL_Delay
  [Called By]
  - >> SetSysClock
  - >> rtc_init

  HAL_RTC_GetDate (Thumb, 124 bytes, Stack size 24 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_GetDate))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_RTC_GetDate ⇒ HAL_RTC_GetTime ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> HAL_RTC_GetTime
  [Called By]
  - >> rtc_read

  HAL_RTC_GetTime (Thumb, 606 bytes, Stack size 32 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_GetTime))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RTC_GetTime ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> RTC_WriteTimeCounter
  - >> RTC_WriteAlarmCounter
  [Called By]
  - >> HAL_RTC_GetDate
  - >> rtc_read

  HAL_RTC_Init (Thumb, 294 bytes, Stack size 24 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_RTC_Init ⇒ HAL_RCCEx_GetPeriphCLKFreq ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_GetTick
  - >> HAL_RTC_MspInit
  - >> HAL_RCCEx_GetPeriphCLKFreq
  [Called By]
  - >> rtc_init

  HAL_RTC_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_MspInit))
  [Called By]

  - >> HAL_RTC_Init

  HAL_RTC_SetDate (Thumb, 362 bytes, Stack size 32 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_SetDate))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RTC_SetDate ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> RTC_WriteTimeCounter
  - >> RTC_WriteAlarmCounter
  [Called By]
  - >> rtc_write

  HAL_RTC_SetTime (Thumb, 220 bytes, Stack size 24 bytes, stm32f1xx_hal_rtc.o(i.HAL_RTC_SetTime))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_RTC_SetTime ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> RTC_WriteTimeCounter
  - >> RTC_WriteAlarmCounter
  [Called By]
  - >> rtc_write

  HAL_SPI_Init (Thumb, 134 bytes, Stack size 8 bytes, stm32f1xx_hal_spi_ex.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SPI_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> init_spi

  HAL_SPI_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_MspInit))
  [Called By]

  - >> HAL_SPI_Init

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> HAL_InitTick

  HAL_TIM_Base_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_MspInit))
  [Called By]

  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Start))
  [Called By]

  - >> HAL_InitTick

  HAL_TIM_OC_Start (Thumb, 54 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_OC_Start))
  [Called By]

  - >> HAL_InitTick

  HAL_UART_Init (Thumb, 94 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> serial_init

  HAL_UART_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_MspInit))
  [Called By]

  - >> HAL_UART_Init

  NVIC_SetVector (Thumb, 102 bytes, Stack size 24 bytes, cmsis_nvic.o(i.NVIC_SetVector))
  [Stack]

  - Max Depth = 32
  - Call Chain = NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> __aeabi_memmove4
  [Called By]
  - >> HAL_InitTick
  - >> gpio_irq_init

  SetSysClock (Thumb, 188 bytes, Stack size 96 bytes, system_stm32f1xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 176
  - Call Chain = SetSysClock ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  [Called By]
  - >> SystemInit

  Set_GPIO_Clock (Thumb, 104 bytes, Stack size 16 bytes, pinmap.o(i.Set_GPIO_Clock))
  [Stack]

  - Max Depth = 112
  - Call Chain = Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> gpio_init
  - >> gpio_irq_init
  - >> pin_mode
  - >> pin_function

  SystemCoreClockUpdate (Thumb, 90 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemCoreClockUpdate))
  [Called By]

  - >> mbed_sdk_init
  - >> HAL_InitTick

  SystemInit (Thumb, 92 bytes, Stack size 8 bytes, system_stm32f1xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 184
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_Init
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(.text)

  TIM_Base_SetConfig (Thumb, 94 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  FATDirHandle::~FATDirHandle__deallocating() (Thumb, 18 bytes, Stack size 16 bytes, fatdirhandle.o(i._ZN12FATDirHandleD0Ev))
  [Stack]

  - Max Depth = 32
  - Call Chain = FATDirHandle::~FATDirHandle__deallocating() ⇒ operator delete (void*) ⇒ free
  [Calls]
  - >> FATDirHandle::~FATDirHandle()
  - >> operator delete (void*)
  [Address Reference Count : 1]
  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::~FATDirHandle() (Thumb, 4 bytes, Stack size 0 bytes, fatdirhandle.o(i._ZN12FATDirHandleD1Ev))
  [Called By]

  - >> FATDirHandle::~FATDirHandle__deallocating()
  [Address Reference Count : 1]
  - fatdirhandle.o(.constdata__ZTV12FATDirHandle)

  FATDirHandle::~FATDirHandle__sub_object() (Thumb, 0 bytes, Stack size 0 bytes, fatdirhandle.o(i._ZN12FATDirHandleD1Ev), UNUSED)

  SDFileSystem::~SDFileSystem() (Thumb, 28 bytes, Stack size 8 bytes, player.o(i._ZN12SDFileSystemD1Ev))
  [Stack]

  - Max Depth = 24
  - Call Chain = SDFileSystem::~SDFileSystem() ⇒ FATFileSystem::~FATFileSystem__sub_object()
  [Calls]
  - >> FATFileSystem::~FATFileSystem__sub_object()
  [Address Reference Count : 2]
  - sdfilesystem.o(.constdata__ZTV12SDFileSystem)
  - player.o(.text)

  SDFileSystem::~SDFileSystem__sub_object() (Thumb, 0 bytes, Stack size 8 bytes, player.o(i._ZN12SDFileSystemD1Ev), UNUSED)

  FATFileHandle::~FATFileHandle__deallocating() (Thumb, 18 bytes, Stack size 16 bytes, fatfilehandle.o(i._ZN13FATFileHandleD0Ev))
  [Stack]

  - Max Depth = 32
  - Call Chain = FATFileHandle::~FATFileHandle__deallocating() ⇒ operator delete (void*) ⇒ free
  [Calls]
  - >> FATFileHandle::~FATFileHandle()
  - >> operator delete (void*)
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::~FATFileHandle() (Thumb, 14 bytes, Stack size 8 bytes, fatfilehandle.o(i._ZN13FATFileHandleD1Ev))
  [Stack]

  - Max Depth = 12
  - Call Chain = FATFileHandle::~FATFileHandle() ⇒ mbed::FileHandle::~FileHandle__sub_object()
  [Calls]
  - >> mbed::FileHandle::~FileHandle__sub_object()
  [Called By]
  - >> FATFileHandle::~FATFileHandle__deallocating()
  [Address Reference Count : 1]
  - fatfilehandle.o(.constdata__ZTV13FATFileHandle)

  FATFileHandle::~FATFileHandle__sub_object() (Thumb, 0 bytes, Stack size 8 bytes, fatfilehandle.o(i._ZN13FATFileHandleD1Ev), UNUSED)

  FATFileSystem::disk_status() (Thumb, 6 bytes, Stack size 0 bytes, fatfilesystem.o(i._ZN13FATFileSystem11disk_statusEv))
  [Address Reference Count : 1]

  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::disk_initialize() (Thumb, 6 bytes, Stack size 0 bytes, fatfilesystem.o(i._ZN13FATFileSystem15disk_initializeEv))
  [Address Reference Count : 1]

  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  FATFileSystem::disk_sync() (Thumb, 6 bytes, Stack size 0 bytes, fatfilesystem.o(i._ZN13FATFileSystem9disk_syncEv))
  [Address Reference Count : 1]

  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)

  mbed::DigitalOut::DigitalOut(PinName) (Thumb, 26 bytes, Stack size 16 bytes, vs10xx.o(i._ZN4mbed10DigitalOutC1E7PinName))
  [Stack]

  - Max Depth = 208
  - Call Chain = mbed::DigitalOut::DigitalOut(PinName) ⇒ gpio_init_out ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_init_out
  - >> __aeabi_memclr4
  [Called By]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  mbed::DigitalOut::DigitalOut__sub_object(PinName) (Thumb, 0 bytes, Stack size 16 bytes, vs10xx.o(i._ZN4mbed10DigitalOutC1E7PinName), UNUSED)

  mbed::DigitalOut::operator =(int) (Thumb, 22 bytes, Stack size 16 bytes, main.o(i._ZN4mbed10DigitalOutaSEi))
  [Stack]

  - Max Depth = 112
  - Call Chain = mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_write(gpio_t*, int)
  [Called By]
  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)
  - >> vs10xx::reset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> LEDflip()
  - >> SDFileSystem::_write(const unsigned char*, unsigned)
  - >> SDFileSystem::initialise_card()
  - >> SDFileSystem::_cmd8()
  - >> SDFileSystem::_cmd58()
  - >> SDFileSystem::_cmdx(int, int)
  - >> SDFileSystem::_read(unsigned char*, unsigned)
  - >> SDFileSystem::_cmd(int, int)

  mbed::FileHandle::~FileHandle() (Thumb, 0 bytes, Stack size 4 bytes, retarget.o(i._ZN4mbed10FileHandleD2Ev), UNUSED)

  mbed::FileHandle::~FileHandle__sub_object() (Thumb, 38 bytes, Stack size 4 bytes, retarget.o(i._ZN4mbed10FileHandleD2Ev))
  [Stack]

  - Max Depth = 4
  - Call Chain = mbed::FileHandle::~FileHandle__sub_object()
  [Called By]
  - >> FATFileHandle::~FATFileHandle()
  [Address Reference Count : 1]
  - retarget.o(.constdata__ZTVN4mbed10FileHandleE)

  mbed::TimerEvent::irq(unsigned) (Thumb, 6 bytes, Stack size 0 bytes, TimerEvent.o(i._ZN4mbed10TimerEvent3irqEj))
  [Address Reference Count : 1]

  - TimerEvent.o(i._ZN4mbed10TimerEventC2Ev)

  mbed::TimerEvent::insert(unsigned) (Thumb, 16 bytes, Stack size 0 bytes, TimerEvent.o(i._ZN4mbed10TimerEvent6insertEj))
  [Stack]

  - Max Depth = 16
  - Call Chain = mbed::TimerEvent::insert(unsigned) ⇒ ticker_insert_event
  [Calls]
  - >> ticker_insert_event
  [Called By]
  - >> mbed::Ticker::setup(unsigned)
  - >> mbed::Ticker::handler()

  mbed::TimerEvent::remove() (Thumb, 10 bytes, Stack size 0 bytes, TimerEvent.o(i._ZN4mbed10TimerEvent6removeEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::TimerEvent::remove() ⇒ ticker_remove_event
  [Calls]
  - >> ticker_remove_event
  [Called By]
  - >> mbed::Ticker::setup(unsigned)
  - >> mbed::Ticker::~Ticker()

  mbed::TimerEvent::TimerEvent__sub_object() (Thumb, 32 bytes, Stack size 8 bytes, TimerEvent.o(i._ZN4mbed10TimerEventC2Ev))
  [Stack]

  - Max Depth = 24
  - Call Chain = mbed::TimerEvent::TimerEvent__sub_object() ⇒ ticker_set_handler
  [Calls]
  - >> ticker_set_handler
  - >> get_us_ticker_data
  [Called By]
  - >> __sti___8_main_cpp

  mbed::TimerEvent::~TimerEvent() (Thumb, 0 bytes, Stack size 8 bytes, TimerEvent.o(i._ZN4mbed10TimerEventD2Ev), UNUSED)

  mbed::TimerEvent::~TimerEvent__sub_object() (Thumb, 20 bytes, Stack size 8 bytes, TimerEvent.o(i._ZN4mbed10TimerEventD2Ev))
  [Stack]

  - Max Depth = 16
  - Call Chain = mbed::TimerEvent::~TimerEvent__sub_object() ⇒ ticker_remove_event
  [Calls]
  - >> ticker_remove_event
  [Called By]
  - >> mbed::Ticker::~Ticker()
  [Address Reference Count : 1]
  - TimerEvent.o(.constdata__ZTVN4mbed10TimerEventE)

  mbed::InterruptIn::_irq_handler(unsigned, gpio_irq_event) (Thumb, 66 bytes, Stack size 0 bytes, InterruptIn.o(i._ZN4mbed11InterruptIn12_irq_handlerEj14gpio_irq_event))
  [Address Reference Count : 1]

  - InterruptIn.o(i._ZN4mbed11InterruptInC1E7PinName)

  mbed::InterruptIn::fall(void(*)()) (Thumb, 28 bytes, Stack size 0 bytes, InterruptIn.o(i._ZN4mbed11InterruptIn4fallEPFvvE))
  [Stack]

  - Max Depth = 168
  - Call Chain = mbed::InterruptIn::fall(void(*)()) ⇒ gpio_irq_set ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_irq_set
  [Called By]
  - >> $Super$$main

  mbed::InterruptIn::rise(void(*)()) (Thumb, 28 bytes, Stack size 0 bytes, InterruptIn.o(i._ZN4mbed11InterruptIn4riseEPFvvE))
  [Stack]

  - Max Depth = 168
  - Call Chain = mbed::InterruptIn::rise(void(*)()) ⇒ gpio_irq_set ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_irq_set
  [Called By]
  - >> $Super$$main

  mbed::InterruptIn::InterruptIn(PinName) (Thumb, 62 bytes, Stack size 16 bytes, InterruptIn.o(i._ZN4mbed11InterruptInC1E7PinName))
  [Stack]

  - Max Depth = 216
  - Call Chain = mbed::InterruptIn::InterruptIn(PinName) ⇒ gpio_irq_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_init_in
  - >> gpio_irq_init
  [Called By]
  - >> __sti___8_main_cpp

  mbed::InterruptIn::InterruptIn__sub_object(PinName) (Thumb, 0 bytes, Stack size 16 bytes, InterruptIn.o(i._ZN4mbed11InterruptInC1E7PinName), UNUSED)

  mbed::InterruptIn::~InterruptIn() (Thumb, 20 bytes, Stack size 8 bytes, InterruptIn.o(i._ZN4mbed11InterruptInD1Ev))
  [Stack]

  - Max Depth = 184
  - Call Chain = mbed::InterruptIn::~InterruptIn() ⇒ gpio_irq_free ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_irq_free
  [Address Reference Count : 2]
  - main.o(.text)
  - InterruptIn.o(.constdata__ZTVN4mbed11InterruptInE)

  mbed::InterruptIn::~InterruptIn__sub_object() (Thumb, 0 bytes, Stack size 8 bytes, InterruptIn.o(i._ZN4mbed11InterruptInD1Ev), UNUSED)

  mbed::InterruptIn::operator int() (Thumb, 38 bytes, Stack size 8 bytes, InterruptIn.o(i._ZN4mbed11InterruptIncviEv))
  [Stack]

  - Max Depth = 88
  - Call Chain = mbed::InterruptIn::operator int() ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  [Called By]
  - >> Pre_Next()
  - >> VolumeFlip()

  mbed::BaseDirHandle::readdir() (Thumb, 44 bytes, Stack size 8 bytes, FileSystemLike.o(i._ZN4mbed13BaseDirHandle7readdirEv))
  [Stack]

  - Max Depth = 16
  - Call Chain = mbed::BaseDirHandle::readdir() ⇒ strncpy
  [Calls]
  - >> mbed::FileBase::getName()
  - >> mbed::FileBase::get(int)
  - >> strncpy
  [Address Reference Count : 1]
  - FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)

  mbed::BaseDirHandle::closedir() (Thumb, 12 bytes, Stack size 8 bytes, FileSystemLike.o(i._ZN4mbed13BaseDirHandle8closedirEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::BaseDirHandle::closedir()
  [Address Reference Count : 1]
  - FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)

  mbed::BaseDirHandle::~BaseDirHandle__deallocating() (Thumb, 4 bytes, Stack size 0 bytes, FileSystemLike.o(i._ZN4mbed13BaseDirHandleD0Ev))
  [Stack]

  - Max Depth = 16
  - Call Chain = mbed::BaseDirHandle::~BaseDirHandle__deallocating() ⇒ operator delete (void*) ⇒ free
  [Calls]
  - >> operator delete (void*)
  [Address Reference Count : 1]
  - FileSystemLike.o(.constdata__ZTVN4mbed13BaseDirHandleE)

  mbed::FileSystemLike::opendir(const char*) (Thumb, 4 bytes, Stack size 0 bytes, FileSystemLike.o(i._ZN4mbed14FileSystemLike7opendirEPKc))
  [Address Reference Count : 1]

  - FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)

  mbed::FileSystemLike::opendir() (Thumb, 34 bytes, Stack size 8 bytes, FileSystemLike.o(i._ZN4mbed14FileSystemLike7opendirEv))
  [Stack]

  - Max Depth = 36
  - Call Chain = mbed::FileSystemLike::opendir() ⇒ operator new(unsigned) ⇒ malloc
  [Calls]
  - >> operator new(unsigned)
  - >> __aeabi_memclr4
  [Called By]
  - >> opendir

  mbed::FileSystemLike::FileSystemLike__sub_object(const char*) (Thumb, 14 bytes, Stack size 8 bytes, FileSystemLike.o(i._ZN4mbed14FileSystemLikeC2EPKc))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FileSystemLike::FileSystemLike__sub_object(const char*)
  [Calls]
  - >> mbed::FileBase::FileBase(const char*, mbed::PathType)
  [Called By]
  - >> FATFileSystem::FATFileSystem__sub_object(const char*)

  mbed::FileSystemLike::~FileSystemLike() (Thumb, 0 bytes, Stack size 0 bytes, FileSystemLike.o(i._ZN4mbed14FileSystemLikeD2Ev), UNUSED)

  mbed::FileSystemLike::~FileSystemLike__sub_object() (Thumb, 4 bytes, Stack size 0 bytes, FileSystemLike.o(i._ZN4mbed14FileSystemLikeD2Ev))
  [Calls]

  - >> mbed::FileBase::~FileBase()
  [Called By]
  - >> FATFileSystem::~FATFileSystem__sub_object()
  [Address Reference Count : 1]
  - FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)

  mbed::SPI::write(int) (Thumb, 48 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPI5writeEi))
  [Stack]

  - Max Depth = 72
  - Call Chain = mbed::SPI::write(int) ⇒ spi_frequency ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> spi_master_write
  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> vs10xx::reset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> SDFileSystem::_write(const unsigned char*, unsigned)
  - >> SDFileSystem::initialise_card()
  - >> SDFileSystem::_cmd8()
  - >> SDFileSystem::_cmd58()
  - >> SDFileSystem::_cmdx(int, int)
  - >> SDFileSystem::_read(unsigned char*, unsigned)
  - >> SDFileSystem::_cmd(int, int)
  [Address Reference Count : 1]
  - SPI.o(.constdata__ZTVN4mbed3SPIE)

  mbed::SPI::frequency(int) (Thumb, 36 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPI9frequencyEi))
  [Stack]

  - Max Depth = 72
  - Call Chain = mbed::SPI::frequency(int) ⇒ spi_frequency ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> vs10xx::setFreq(int)
  - >> vs10xx::softReset()
  - >> SDFileSystem::disk_initialize()
  - >> SDFileSystem::initialise_card()

  mbed::SPI::SPI(PinName, PinName, PinName, PinName) (Thumb, 74 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPIC1E7PinNameS1_S1_S1_))
  [Stack]

  - Max Depth = 224
  - Call Chain = mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> spi_init
  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  mbed::SPI::SPI__sub_object(PinName, PinName, PinName, PinName) (Thumb, 0 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPIC1E7PinNameS1_S1_S1_), UNUSED)

  mbed::Timer::start() (Thumb, 26 bytes, Stack size 8 bytes, Timer.o(i._ZN4mbed5Timer5startEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::Timer::start()
  [Calls]
  - >> ticker_read
  [Called By]
  - >> $Super$$main

  mbed::Timer::read_ms() (Thumb, 32 bytes, Stack size 8 bytes, Timer.o(i._ZN4mbed5Timer7read_msEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::Timer::read_ms()
  [Calls]
  - >> ticker_read
  [Called By]
  - >> riseFlip()
  - >> fallFlip()

  mbed::Timer::Timer() (Thumb, 30 bytes, Stack size 16 bytes, Timer.o(i._ZN4mbed5TimerC1Ev))
  [Stack]

  - Max Depth = 16
  - Call Chain = mbed::Timer::Timer()
  [Calls]
  - >> get_us_ticker_data
  - >> ticker_read
  [Called By]
  - >> __sti___8_main_cpp

  mbed::Timer::Timer__sub_object() (Thumb, 0 bytes, Stack size 16 bytes, Timer.o(i._ZN4mbed5TimerC1Ev), UNUSED)

  mbed::Ticker::setup(unsigned) (Thumb, 32 bytes, Stack size 16 bytes, Ticker.o(i._ZN4mbed6Ticker5setupEj))
  [Stack]

  - Max Depth = 32
  - Call Chain = mbed::Ticker::setup(unsigned) ⇒ mbed::TimerEvent::insert(unsigned) ⇒ ticker_insert_event
  [Calls]
  - >> ticker_read
  - >> mbed::TimerEvent::remove()
  - >> mbed::TimerEvent::insert(unsigned)
  [Called By]
  - >> $Super$$main

  mbed::Ticker::handler() (Thumb, 52 bytes, Stack size 8 bytes, Ticker.o(i._ZN4mbed6Ticker7handlerEv))
  [Stack]

  - Max Depth = 24
  - Call Chain = mbed::Ticker::handler() ⇒ mbed::TimerEvent::insert(unsigned) ⇒ ticker_insert_event
  [Calls]
  - >> mbed::TimerEvent::insert(unsigned)
  [Address Reference Count : 1]
  - Ticker.o(.constdata__ZTVN4mbed6TickerE)

  mbed::Ticker::~Ticker() (Thumb, 30 bytes, Stack size 8 bytes, Ticker.o(i._ZN4mbed6TickerD1Ev))
  [Stack]

  - Max Depth = 24
  - Call Chain = mbed::Ticker::~Ticker() ⇒ mbed::TimerEvent::~TimerEvent__sub_object() ⇒ ticker_remove_event
  [Calls]
  - >> mbed::TimerEvent::~TimerEvent__sub_object()
  - >> mbed::TimerEvent::remove()
  [Address Reference Count : 2]
  - main.o(.text)
  - Ticker.o(.constdata__ZTVN4mbed6TickerE)

  mbed::Ticker::~Ticker__sub_object() (Thumb, 0 bytes, Stack size 8 bytes, Ticker.o(i._ZN4mbed6TickerD1Ev), UNUSED)

  mbed::FileBase::getPathType() (Thumb, 4 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBase11getPathTypeEv))
  [Called By]

  - >> mbed::FilePath::isFile()
  - >> mbed::FilePath::file()
  - >> mbed::FilePath::fileSystem()

  mbed::FileBase::get(int) (Thumb, 28 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBase3getEi))
  [Called By]

  - >> mbed::BaseDirHandle::readdir()

  mbed::FileBase::lookup(const char*, unsigned) (Thumb, 50 bytes, Stack size 16 bytes, FileBase.o(i._ZN4mbed8FileBase6lookupEPKcj))
  [Stack]

  - Max Depth = 28
  - Call Chain = mbed::FileBase::lookup(const char*, unsigned) ⇒ strncmp
  [Calls]
  - >> strncmp
  - >> strlen
  [Called By]
  - >> mbed::FilePath::FilePath(const char*)

  mbed::FileBase::getName() (Thumb, 4 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBase7getNameEv))
  [Called By]

  - >> mbed::BaseDirHandle::readdir()

  mbed::FileBase::FileBase(const char*, mbed::PathType) (Thumb, 28 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBaseC1EPKcNS_8PathTypeE))
  [Called By]

  - >> mbed::FileSystemLike::FileSystemLike__sub_object(const char*)

  mbed::FileBase::FileBase__sub_object(const char*, mbed::PathType) (Thumb, 0 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBaseC1EPKcNS_8PathTypeE), UNUSED)

  mbed::FileBase::~FileBase() (Thumb, 46 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBaseD1Ev))
  [Called By]

  - >> mbed::FileSystemLike::~FileSystemLike__sub_object()
  [Address Reference Count : 1]
  - FileBase.o(.constdata__ZTVN4mbed8FileBaseE)

  mbed::FileBase::~FileBase__sub_object() (Thumb, 0 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBaseD1Ev), UNUSED)

  mbed::FilePath::fileSystem() (Thumb, 24 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath10fileSystemEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::fileSystem()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> opendir
  - >> _sys_open

  mbed::FilePath::file() (Thumb, 28 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath4fileEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::file()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> _sys_open

  mbed::FilePath::exists() (Thumb, 10 bytes, Stack size 0 bytes, FilePath.o(i._ZN4mbed8FilePath6existsEv))
  [Called By]

  - >> _sys_open

  mbed::FilePath::isFile() (Thumb, 24 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath6isFileEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::isFile()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> _sys_open

  mbed::FilePath::fileName() (Thumb, 4 bytes, Stack size 0 bytes, FilePath.o(i._ZN4mbed8FilePath8fileNameEv))
  [Called By]

  - >> opendir
  - >> _sys_open

  mbed::FilePath::FilePath(const char*) (Thumb, 64 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePathC1EPKc))
  [Stack]

  - Max Depth = 36
  - Call Chain = mbed::FilePath::FilePath(const char*) ⇒ mbed::FileBase::lookup(const char*, unsigned) ⇒ strncmp
  [Calls]
  - >> mbed::FileBase::lookup(const char*, unsigned)
  [Called By]
  - >> opendir
  - >> _sys_open

  mbed::FilePath::FilePath__sub_object(const char*) (Thumb, 0 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePathC1EPKc), UNUSED)

  mbed::DigitalIn::operator int() (Thumb, 52 bytes, Stack size 8 bytes, vs10xx.o(i._ZN4mbed9DigitalIncviEv))
  [Stack]

  - Max Depth = 88
  - Call Chain = mbed::DigitalIn::operator int() ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  [Called By]
  - >> vs10xx::softReset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)

  vs10xx::~vs10xx() (Thumb, 4 bytes, Stack size 0 bytes, player.o(i._ZN6vs10xxD1Ev))
  [Address Reference Count : 1]

  - player.o(.text)

  vs10xx::~vs10xx__sub_object() (Thumb, 0 bytes, Stack size 0 bytes, player.o(i._ZN6vs10xxD1Ev), UNUSED)

  std::strstr(char*, const char*) (Thumb, 16 bytes, Stack size 16 bytes, player.o(i._ZSt6strstrPcPKc))
  [Stack]

  - Max Depth = 28
  - Call Chain = std::strstr(char*, const char*) ⇒ strstr
  [Calls]
  - >> strstr
  [Called By]
  - >> Player::playFile(char*)
  - >> Player::begin()

  operator delete (void*) (Thumb, 8 bytes, Stack size 8 bytes, delete.o(i._ZdlPv))
  [Stack]

  - Max Depth = 16
  - Call Chain = operator delete (void*) ⇒ free
  [Calls]
  - >> free
  [Called By]
  - >> FATFileSystem::~FATFileSystem__deallocating()
  - >> FATFileHandle::~FATFileHandle__deallocating()
  - >> FATDirHandle::~FATDirHandle__deallocating()
  - >> mbed::BaseDirHandle::~BaseDirHandle__deallocating()

  operator new(unsigned) (Thumb, 34 bytes, Stack size 8 bytes, new.o(i._Znwj))
  [Stack]

  - Max Depth = 28
  - Call Chain = operator new(unsigned) ⇒ malloc
  [Calls]
  - >> malloc
  - >> __rt_new_handler_addr
  [Called By]
  - >> FATFileSystem::open(const char*, int)
  - >> mbed::FileSystemLike::opendir()
  - >> FATFileSystem::opendir(const char*)

  __0fprintf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)
  [Calls]

  - >> _printf_core

  __1fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  __2fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2fprintf
  [Called By]
  - >> mbed_assert_internal

  __c89fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> vs10xx::softReset()
  - >> Player::playFile(char*)
  - >> Player::begin()
  - >> Player::recordFile(char*)
  - >> VolumeFlip()

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> FATFileSystem::open(const char*, int)

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __0vfprintf (Thumb, 20 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)
  [Calls]

  - >> _printf_core

  __1vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)

  __2vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)

  __c89vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf))
  [Stack]

  - Max Depth = 8
  - Call Chain = __c89vfprintf
  [Called By]
  - >> debug(const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> debug_if(int, const char*, ...)
  - >> debug_if(int, const char*, ...)

  vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf))
  [Stack]

  - Max Depth = 8
  - Call Chain = vfprintf
  [Called By]
  - >> error

  __aeabi_atexit (Thumb, 50 bytes, Stack size 24 bytes, aeabi_atexit.o(i.__aeabi_atexit))
  [Stack]

  - Max Depth = 44
  - Call Chain = __aeabi_atexit ⇒ malloc
  [Calls]
  - >> malloc
  - >> __rt_ddtor_pointer_addr
  [Called By]
  - >> __sti___10_player_cpp
  - >> __sti___8_main_cpp

  __cxa_finalize (Thumb, 66 bytes, Stack size 24 bytes, cxa_finalize.o(i.__cxa_finalize), UNUSED)
  [Calls]

  - >> free
  - >> __rt_ddtor_pointer_addr

  __cxa_pure_virtual (Thumb, 6 bytes, Stack size 0 bytes, pure_virt.o(i.__cxa_pure_virtual))
  [Calls]

  - >> __rt_SIGPVFN
  [Address Reference Count : 5]
  - fatdirhandle.o(.constdata__ZTVN4mbed9DirHandleE)
  - fatfilesystem.o(.constdata__ZTV13FATFileSystem)
  - retarget.o(.constdata__ZTVN4mbed10FileHandleE)
  - FileSystemLike.o(.constdata__ZTVN4mbed14FileSystemLikeE)
  - TimerEvent.o(.constdata__ZTVN4mbed10TimerEventE)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  _sys_ensure (Thumb, 34 bytes, Stack size 0 bytes, retarget.o(i._sys_ensure))
  [Called By]

  - >> fflush

  _sys_open (Thumb, 212 bytes, Stack size 32 bytes, retarget.o(i._sys_open))
  [Stack]

  - Max Depth = 248
  - Call Chain = _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> mbed::FilePath::FilePath(const char*)
  - >> mbed::FilePath::fileName()
  - >> mbed::FilePath::isFile()
  - >> mbed::FilePath::exists()
  - >> mbed::FilePath::file()
  - >> mbed::FilePath::fileSystem()
  - >> __0sscanf
  - >> strcmp
  [Called By]
  - >> _initio

  _sys_seek (Thumb, 36 bytes, Stack size 0 bytes, retarget.o(i._sys_seek))
  [Called By]

  - >> fflush

  _sys_write (Thumb, 82 bytes, Stack size 16 bytes, retarget.o(i._sys_write))
  [Stack]

  - Max Depth = 216
  - Call Chain = _sys_write ⇒ serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> serial_putc
  - >> serial_init
  [Called By]
  - >> fputc

  error (Thumb, 20 bytes, Stack size 24 bytes, error.o(i.error))
  [Stack]

  - Max Depth = 96
  - Call Chain = error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> exit
  - >> vfprintf
  [Called By]
  - >> FATFileSystem::FATFileSystem__sub_object(const char*)
  - >> Set_GPIO_Clock
  - >> rtc_init
  - >> gpio_irq_init
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge

  exit (Thumb, 24 bytes, Stack size 0 bytes, retarget.o(i.exit))
  [Stack]

  - Max Depth = 72
  - Call Chain = exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_die
  - >> fflush
  [Called By]
  - >> error

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free))
  [Stack]

  - Max Depth = 8
  - Call Chain = free
  [Called By]
  - >> operator delete (void*)
  - >> __cxa_finalize

  get_us_ticker_data (Thumb, 4 bytes, Stack size 0 bytes, us_ticker_api.o(i.get_us_ticker_data))
  [Called By]

  - >> mbed::Timer::Timer()
  - >> mbed::TimerEvent::TimerEvent__sub_object()

  gpio_dir (Thumb, 52 bytes, Stack size 16 bytes, gpio_api.o(i.gpio_dir))
  [Stack]

  - Max Depth = 176
  - Call Chain = gpio_dir ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> pin_function
  [Called By]
  - >> gpio_init_in
  - >> gpio_init_out

  gpio_init (Thumb, 60 bytes, Stack size 16 bytes, gpio_api.o(i.gpio_init))
  [Stack]

  - Max Depth = 176
  - Call Chain = gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> Set_GPIO_Clock
  - >> pin_function
  [Called By]
  - >> gpio_init_in
  - >> gpio_init_out

  gpio_init_in (Thumb, 38 bytes, Stack size 16 bytes, gpio.o(i.gpio_init_in))
  [Stack]

  - Max Depth = 192
  - Call Chain = gpio_init_in ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_init
  - >> gpio_dir
  - >> gpio_mode
  [Called By]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> mbed::InterruptIn::InterruptIn(PinName)

  gpio_init_out (Thumb, 64 bytes, Stack size 16 bytes, gpio.o(i.gpio_init_out))
  [Stack]

  - Max Depth = 192
  - Call Chain = gpio_init_out ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> gpio_init
  - >> gpio_dir
  - >> gpio_mode
  [Called By]
  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)
  - >> mbed::DigitalOut::DigitalOut(PinName)
  - >> __sti___8_main_cpp

  gpio_irq_free (Thumb, 68 bytes, Stack size 16 bytes, gpio_irq_api.o(i.gpio_irq_free))
  [Stack]

  - Max Depth = 176
  - Call Chain = gpio_irq_free ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> pin_function
  [Called By]
  - >> mbed::InterruptIn::~InterruptIn()

  gpio_irq_init (Thumb, 252 bytes, Stack size 40 bytes, gpio_irq_api.o(i.gpio_irq_init))
  [Stack]

  - Max Depth = 200
  - Call Chain = gpio_irq_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  - >> NVIC_SetVector
  - >> Set_GPIO_Clock
  - >> pin_function
  [Called By]
  - >> mbed::InterruptIn::InterruptIn(PinName)

  gpio_irq_set (Thumb, 114 bytes, Stack size 8 bytes, gpio_irq_api.o(i.gpio_irq_set))
  [Stack]

  - Max Depth = 168
  - Call Chain = gpio_irq_set ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> pin_function
  [Called By]
  - >> mbed::InterruptIn::rise(void(*)())
  - >> mbed::InterruptIn::fall(void(*)())

  gpio_mode (Thumb, 8 bytes, Stack size 0 bytes, gpio_api.o(i.gpio_mode))
  [Stack]

  - Max Depth = 144
  - Call Chain = gpio_mode ⇒ pin_mode ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> pin_mode
  [Called By]
  - >> gpio_init_in
  - >> gpio_init_out

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> __aeabi_atexit
  - >> operator new(unsigned)
  - >> __ARM_exceptions_buffer_init
  - >> __cxa_get_globals

  mbed_assert_internal (Thumb, 24 bytes, Stack size 8 bytes, assert.o(i.mbed_assert_internal))
  [Stack]

  - Max Depth = 80
  - Call Chain = mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_die
  - >> __2fprintf
  [Called By]
  - >> gpio_write(gpio_t*, int)
  - >> mbed::DigitalIn::operator int()
  - >> gpio_write(gpio_t*, int)
  - >> gpio_init_out
  - >> mbed::InterruptIn::operator int()
  - >> LEDflip()
  - >> gpio_write(gpio_t*, int)
  - >> serial_init
  - >> gpio_dir
  - >> spi_init
  - >> pin_mode
  - >> pin_function

  mbed_die (Thumb, 16 bytes, Stack size 0 bytes, board.o(i.mbed_die))
  [Stack]

  - Max Depth = 72
  - Call Chain = mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> wait_ms
  [Called By]
  - >> mbed_assert_internal
  - >> exit

  mbed_main (Thumb, 2 bytes, Stack size 0 bytes, retarget.o(i.mbed_main))
  [Called By]

  - >> main

  mbed_sdk_init (Thumb, 14 bytes, Stack size 8 bytes, mbed_overrides.o(i.mbed_sdk_init))
  [Stack]

  - Max Depth = 64
  - Call Chain = mbed_sdk_init ⇒ HAL_Init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SystemCoreClockUpdate
  - >> HAL_Init
  [Called By]
  - >> main

  opendir (Thumb, 68 bytes, Stack size 16 bytes, retarget.o(i.opendir))
  [Stack]

  - Max Depth = 52
  - Call Chain = opendir ⇒ mbed::FilePath::FilePath(const char*) ⇒ mbed::FileBase::lookup(const char*, unsigned) ⇒ strncmp
  [Calls]
  - >> mbed::FilePath::FilePath(const char*)
  - >> mbed::FilePath::fileName()
  - >> mbed::FilePath::fileSystem()
  - >> mbed::FileSystemLike::opendir()
  [Called By]
  - >> Player::begin()

  pin_function (Thumb, 256 bytes, Stack size 48 bytes, pinmap.o(i.pin_function))
  [Stack]

  - Max Depth = 160
  - Call Chain = pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> HAL_GPIO_Init
  - >> Set_GPIO_Clock
  [Called By]
  - >> gpio_init
  - >> gpio_dir
  - >> gpio_irq_set
  - >> gpio_irq_init
  - >> gpio_irq_free
  - >> pinmap_pinout

  pin_mode (Thumb, 236 bytes, Stack size 32 bytes, pinmap.o(i.pin_mode))
  [Stack]

  - Max Depth = 144
  - Call Chain = pin_mode ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> Set_GPIO_Clock
  [Called By]
  - >> serial_init
  - >> gpio_mode
  - >> pinmap_pinout

  pinmap_merge (Thumb, 34 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_merge))
  [Stack]

  - Max Depth = 104
  - Call Chain = pinmap_merge ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> serial_init
  - >> spi_init

  pinmap_peripheral (Thumb, 58 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_peripheral))
  [Stack]

  - Max Depth = 104
  - Call Chain = pinmap_peripheral ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> serial_init
  - >> spi_init

  pinmap_pinout (Thumb, 66 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_pinout))
  [Stack]

  - Max Depth = 168
  - Call Chain = pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  - >> pin_mode
  - >> pin_function
  [Called By]
  - >> serial_init
  - >> spi_init

  rtc_init (Thumb, 196 bytes, Stack size 72 bytes, rtc_api.o(i.rtc_init))
  [Stack]

  - Max Depth = 168
  - Call Chain = rtc_init ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  - >> HAL_RTC_Init
  - >> HAL_PWR_EnableBkUpAccess
  - >> HAL_RCC_OscConfig
  [Address Reference Count : 1]
  - rtc_time.o(.data)

  rtc_isenabled (Thumb, 6 bytes, Stack size 0 bytes, rtc_api.o(i.rtc_isenabled))
  [Address Reference Count : 1]

  - rtc_time.o(.data)

  rtc_read (Thumb, 86 bytes, Stack size 56 bytes, rtc_api.o(i.rtc_read))
  [Stack]

  - Max Depth = 136
  - Call Chain = rtc_read ⇒ HAL_RTC_GetDate ⇒ HAL_RTC_GetTime ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> HAL_RTC_GetTime
  - >> HAL_RTC_GetDate
  - >> mktime
  [Address Reference Count : 1]
  - rtc_time.o(.data)

  rtc_write (Thumb, 86 bytes, Stack size 16 bytes, rtc_api.o(i.rtc_write))
  [Stack]

  - Max Depth = 72
  - Call Chain = rtc_write ⇒ HAL_RTC_SetDate ⇒ RTC_WriteTimeCounter
  [Calls]
  - >> HAL_RTC_SetTime
  - >> HAL_RTC_SetDate
  - >> localtime
  [Address Reference Count : 1]
  - rtc_time.o(.data)

  serial_init (Thumb, 314 bytes, Stack size 32 bytes, serial_api.o(i.serial_init))
  [Stack]

  - Max Depth = 200
  - Call Chain = serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> HAL_UART_Init
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge
  - >> pin_mode
  [Called By]
  - >> _sys_write

  serial_putc (Thumb, 38 bytes, Stack size 0 bytes, serial_api.o(i.serial_putc))
  [Called By]

  - >> _sys_write

  set_compare (Thumb, 18 bytes, Stack size 0 bytes, us_ticker.o(i.set_compare))
  [Called By]

  - >> timer_irq_handler

  spi_format (Thumb, 102 bytes, Stack size 8 bytes, spi_api.o(i.spi_format))
  [Stack]

  - Max Depth = 24
  - Call Chain = spi_format ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> init_spi
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::SPI::frequency(int)
  - >> mbed::SPI::write(int)

  spi_frequency (Thumb, 232 bytes, Stack size 40 bytes, spi_api.o(i.spi_frequency))
  [Stack]

  - Max Depth = 56
  - Call Chain = spi_frequency ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> init_spi
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::SPI::frequency(int)
  - >> mbed::SPI::write(int)

  spi_init (Thumb, 230 bytes, Stack size 40 bytes, spi_api.o(i.spi_init))
  [Stack]

  - Max Depth = 208
  - Call Chain = spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> init_spi
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)

  spi_master_write (Thumb, 68 bytes, Stack size 0 bytes, spi_api.o(i.spi_master_write))
  [Called By]

  - >> mbed::SPI::write(int)

  ticker_insert_event (Thumb, 62 bytes, Stack size 16 bytes, ticker_api.o(i.ticker_insert_event))
  [Stack]

  - Max Depth = 16
  - Call Chain = ticker_insert_event
  [Called By]
  - >> mbed::TimerEvent::insert(unsigned)

  ticker_irq_handler (Thumb, 78 bytes, Stack size 8 bytes, ticker_api.o(i.ticker_irq_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ticker_irq_handler
  [Called By]
  - >> us_ticker_irq_handler

  ticker_read (Thumb, 6 bytes, Stack size 0 bytes, ticker_api.o(i.ticker_read))
  [Called By]

  - >> mbed::Ticker::setup(unsigned)
  - >> mbed::Timer::Timer()
  - >> mbed::Timer::read_ms()
  - >> mbed::Timer::start()

  ticker_remove_event (Thumb, 60 bytes, Stack size 8 bytes, ticker_api.o(i.ticker_remove_event))
  [Stack]

  - Max Depth = 8
  - Call Chain = ticker_remove_event
  [Called By]
  - >> mbed::TimerEvent::~TimerEvent__sub_object()
  - >> mbed::TimerEvent::remove()

  ticker_set_handler (Thumb, 18 bytes, Stack size 16 bytes, ticker_api.o(i.ticker_set_handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = ticker_set_handler
  [Called By]
  - >> mbed::TimerEvent::TimerEvent__sub_object()

  time (Thumb, 54 bytes, Stack size 16 bytes, rtc_time.o(i.time))
  [Stack]

  - Max Depth = 16
  - Call Chain = time
  [Called By]
  - >> get_fattime

  timer_irq_handler (Thumb, 158 bytes, Stack size 24 bytes, hal_tick.o(i.timer_irq_handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = timer_irq_handler ⇒ us_ticker_irq_handler ⇒ ticker_irq_handler
  [Calls]
  - >> us_ticker_irq_handler
  - >> set_compare
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - hal_tick.o(i.HAL_InitTick)

  us_ticker_clear_interrupt (Thumb, 22 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_clear_interrupt))
  [Address Reference Count : 1]

  - us_ticker_api.o(.constdata)

  us_ticker_disable_interrupt (Thumb, 16 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_disable_interrupt))
  [Address Reference Count : 1]

  - us_ticker_api.o(.constdata)

  us_ticker_init (Thumb, 20 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_init))
  [Stack]

  - Max Depth = 48
  - Call Chain = us_ticker_init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_InitTick
  [Address Reference Count : 1]
  - us_ticker_api.o(.constdata)

  us_ticker_irq_handler (Thumb, 6 bytes, Stack size 0 bytes, us_ticker_api.o(i.us_ticker_irq_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = us_ticker_irq_handler ⇒ ticker_irq_handler
  [Calls]
  - >> ticker_irq_handler
  [Called By]
  - >> timer_irq_handler
  - >> us_ticker_set_interrupt

  us_ticker_read (Thumb, 46 bytes, Stack size 8 bytes, us_ticker.o(i.us_ticker_read))
  [Stack]

  - Max Depth = 56
  - Call Chain = us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_InitTick
  [Called By]
  - >> wait_ms
  [Address Reference Count : 1]
  - us_ticker_api.o(.constdata)

  us_ticker_set_interrupt (Thumb, 134 bytes, Stack size 16 bytes, us_ticker.o(i.us_ticker_set_interrupt))
  [Stack]

  - Max Depth = 64
  - Call Chain = us_ticker_set_interrupt ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> us_ticker_irq_handler
  - >> HAL_InitTick
  [Address Reference Count : 1]
  - us_ticker_api.o(.constdata)

  wait_ms (Thumb, 28 bytes, Stack size 16 bytes, wait_api.o(i.wait_ms))
  [Stack]

  - Max Depth = 72
  - Call Chain = wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> us_ticker_read
  [Called By]
  - >> vs10xx::reset()
  - >> vs10xx::softReset()
  - >> mbed_die
  - >> SDFileSystem::initialise_card_v2()

  mbed::FunctionPointerArg1⟨void, void⟩::attach(void(*)()) (Thumb, 8 bytes, Stack size 0 bytes, main.o(t._ZN4mbed19FunctionPointerArg1IvvE6attachEPFvvE))
  [Called By]

  - >> __sti___8_main_cpp
  - >> $Super$$main

  ### Local Symbols

  __sti___8_main_cpp (Thumb, 174 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 240
  - Call Chain = __sti___8_main_cpp ⇒ mbed::InterruptIn::InterruptIn(PinName) ⇒ gpio_irq_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::FunctionPointerArg1⟨void, void⟩::attach(void(*)())
  - >> gpio_init_out
  - >> mbed::Timer::Timer()
  - >> mbed::InterruptIn::InterruptIn(PinName)
  - >> mbed::TimerEvent::TimerEvent__sub_object()
  - >> __aeabi_atexit
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - main.o(.init_array)

  gpio_write(gpio_t*, int) (Thumb, 46 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  [Called By]
  - >> mbed::DigitalOut::operator =(int)

  gpio_write(gpio_t*, int) (Thumb, 46 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed_assert_internal

  __sti___10_player_cpp (Thumb, 72 bytes, Stack size 24 bytes, player.o(.text))
  [Stack]

  - Max Depth = 288
  - Call Chain = __sti___10_player_cpp ⇒ SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SDFileSystem::SDFileSystem(PinName, PinName, PinName, PinName, const char*)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> __aeabi_atexit
  [Address Reference Count : 1]
  - player.o(.init_array)

  debug_if(int, const char*, ...) (Thumb, 36 bytes, Stack size 32 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> __c89vfprintf
  [Called By]
  - >> SDFileSystem::disk_initialize()
  - >> SDFileSystem::initialise_card_v2()
  - >> SDFileSystem::initialise_card_v1()
  - >> SDFileSystem::_sd_sectors()

  ext_bits(unsigned char*, int, int) (Thumb, 62 bytes, Stack size 28 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = ext_bits(unsigned char*, int, int)
  [Called By]
  - >> SDFileSystem::_sd_sectors()

  debug(const char*, ...) (Thumb, 28 bytes, Stack size 24 bytes, sdfilesystem.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = debug(const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> __c89vfprintf
  [Called By]
  - >> SDFileSystem::disk_initialize()
  - >> SDFileSystem::initialise_card()
  - >> SDFileSystem::initialise_card_v2()
  - >> SDFileSystem::initialise_card_v1()
  - >> SDFileSystem::_sd_sectors()

  gpio_write(gpio_t*, int) (Thumb, 46 bytes, Stack size 16 bytes, sdfilesystem.o(.text), UNUSED)
  [Calls]

  - >> mbed_assert_internal

  debug_if(int, const char*, ...) (Thumb, 36 bytes, Stack size 32 bytes, fatfilehandle.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> __c89vfprintf
  [Called By]
  - >> FATFileHandle::fsync()
  - >> FATFileHandle::lseek(long, int)
  - >> FATFileHandle::read(void*, unsigned)
  - >> FATFileHandle::write(const void*, unsigned)

  debug_if(int, const char*, ...) (Thumb, 36 bytes, Stack size 32 bytes, fatfilesystem.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> __c89vfprintf
  [Called By]
  - >> FATFileSystem::remove(const char*)
  - >> FATFileSystem::open(const char*, int)
  - >> FATFileSystem::FATFileSystem__sub_object(const char*)
  - >> FATFileSystem::format()

  debug_if(int, const char*, ...) (Thumb, 36 bytes, Stack size 32 bytes, diskio.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> __c89vfprintf
  [Called By]
  - >> disk_ioctl(unsigned char, unsigned char, void*)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  - >> disk_status(unsigned char)
  - >> disk_initialize(unsigned char)

  mem_cpy(void*, const void*, unsigned) (Thumb, 26 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = mem_cpy(void*, const void*, unsigned)
  [Called By]
  - >> f_rename
  - >> gen_numname(unsigned char*, const unsigned char*, const unsigned short*, unsigned short)
  - >> dir_register(FATFS_DIR*)
  - >> f_unlink
  - >> f_mkfs
  - >> f_mkdir
  - >> f_write
  - >> f_read

  mem_set(void*, int, unsigned) (Thumb, 20 bytes, Stack size 12 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = mem_set(void*, int, unsigned)
  [Called By]
  - >> create_name(FATFS_DIR*, const char**)
  - >> dir_register(FATFS_DIR*)
  - >> dir_next(FATFS_DIR*, int)
  - >> sync(FATFS*)
  - >> f_mkfs
  - >> f_mkdir

  mem_cmp(const void*, const void*, unsigned) (Thumb, 38 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = mem_cmp(const void*, const void*, unsigned)
  [Called By]
  - >> dir_find(FATFS_DIR*)

  chk_chr(const char*, int) (Thumb, 20 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> create_name(FATFS_DIR*, const char**)

  move_window(FATFS*, unsigned long) (Thumb, 114 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> f_rename
  - >> f_getfree
  - >> put_fat(FATFS*, unsigned long, unsigned long)
  - >> get_fat(FATFS*, unsigned long)
  - >> dir_remove(FATFS_DIR*)
  - >> dir_register(FATFS_DIR*)
  - >> dir_read(FATFS_DIR*)
  - >> dir_find(FATFS_DIR*)
  - >> dir_next(FATFS_DIR*, int)
  - >> sync(FATFS*)
  - >> f_open
  - >> f_mkdir
  - >> f_sync

  sync(FATFS*) (Thumb, 202 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = sync(FATFS*) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> move_window(FATFS*, unsigned long)
  - >> mem_set(void*, int, unsigned)
  - >> disk_ioctl(unsigned char, unsigned char, void*)
  - >> disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_unlink
  - >> f_mkdir
  - >> f_sync

  remove_chain(FATFS*, unsigned long) (Thumb, 104 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = remove_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> put_fat(FATFS*, unsigned long, unsigned long)
  - >> get_fat(FATFS*, unsigned long)
  [Called By]
  - >> f_truncate
  - >> f_unlink
  - >> f_open
  - >> f_mkdir

  create_chain(FATFS*, unsigned long) (Thumb, 202 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> put_fat(FATFS*, unsigned long, unsigned long)
  - >> get_fat(FATFS*, unsigned long)
  [Called By]
  - >> dir_next(FATFS_DIR*, int)
  - >> f_mkdir
  - >> f_write
  - >> f_lseek

  dir_sdi(FATFS_DIR*, unsigned short) (Thumb, 156 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = dir_sdi(FATFS_DIR*, unsigned short) ⇒ get_fat(FATFS*, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> get_fat(FATFS*, unsigned long)
  - >> clust2sect(FATFS*, unsigned long)
  [Called By]
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_remove(FATFS_DIR*)
  - >> dir_register(FATFS_DIR*)
  - >> dir_find(FATFS_DIR*)
  - >> f_unlink
  - >> f_opendir
  - >> f_readdir

  dir_next(FATFS_DIR*, int) (Thumb, 276 bytes, Stack size 24 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 184
  - Call Chain = dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> get_fat(FATFS*, unsigned long)
  - >> clust2sect(FATFS*, unsigned long)
  - >> create_chain(FATFS*, unsigned long)
  - >> move_window(FATFS*, unsigned long)
  - >> mem_set(void*, int, unsigned)
  [Called By]
  - >> dir_remove(FATFS_DIR*)
  - >> dir_register(FATFS_DIR*)
  - >> dir_read(FATFS_DIR*)
  - >> dir_find(FATFS_DIR*)
  - >> f_readdir

  ld_clust(FATFS*, unsigned char*) (Thumb, 32 bytes, Stack size 8 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ld_clust(FATFS*, unsigned char*)
  [Called By]
  - >> f_rename
  - >> follow_path(FATFS_DIR*, const char*)
  - >> f_unlink
  - >> f_opendir
  - >> f_open

  st_clust(unsigned char*, unsigned long) (Thumb, 16 bytes, Stack size 0 bytes, ff.o(.text))
  [Called By]

  - >> f_rename
  - >> f_open
  - >> f_mkdir
  - >> f_sync

  cmp_lfn(unsigned short*, unsigned char*) (Thumb, 138 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = cmp_lfn(unsigned short*, unsigned char*)
  [Calls]
  - >> ff_wtoupper
  [Called By]
  - >> dir_find(FATFS_DIR*)

  pick_lfn(unsigned short*, unsigned char*) (Thumb, 112 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = pick_lfn(unsigned short*, unsigned char*)
  [Called By]
  - >> dir_read(FATFS_DIR*)

  fit_lfn(const unsigned short*, unsigned char*, unsigned char, unsigned char) (Thumb, 122 bytes, Stack size 20 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = fit_lfn(const unsigned short*, unsigned char*, unsigned char, unsigned char)
  [Called By]
  - >> dir_register(FATFS_DIR*)

  sum_sfn(const unsigned char*) (Thumb, 32 bytes, Stack size 12 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = sum_sfn(const unsigned char*)
  [Called By]
  - >> dir_register(FATFS_DIR*)
  - >> dir_read(FATFS_DIR*)
  - >> dir_find(FATFS_DIR*)

  dir_find(FATFS_DIR*) (Thumb, 222 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> sum_sfn(const unsigned char*)
  - >> cmp_lfn(unsigned short*, unsigned char*)
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> move_window(FATFS*, unsigned long)
  - >> mem_cmp(const void*, const void*, unsigned)
  [Called By]
  - >> follow_path(FATFS_DIR*, const char*)
  - >> dir_register(FATFS_DIR*)

  dir_read(FATFS_DIR*) (Thumb, 190 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = dir_read(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> sum_sfn(const unsigned char*)
  - >> pick_lfn(unsigned short*, unsigned char*)
  - >> dir_next(FATFS_DIR*, int)
  - >> move_window(FATFS*, unsigned long)
  [Called By]
  - >> f_unlink
  - >> f_readdir

  dir_register(FATFS_DIR*) (Thumb, 400 bytes, Stack size 56 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 272
  - Call Chain = dir_register(FATFS_DIR*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> gen_numname(unsigned char*, const unsigned char*, const unsigned short*, unsigned short)
  - >> dir_find(FATFS_DIR*)
  - >> sum_sfn(const unsigned char*)
  - >> fit_lfn(const unsigned short*, unsigned char*, unsigned char, unsigned char)
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> move_window(FATFS*, unsigned long)
  - >> mem_set(void*, int, unsigned)
  - >> mem_cpy(void*, const void*, unsigned)
  [Called By]
  - >> f_rename
  - >> f_open
  - >> f_mkdir

  dir_remove(FATFS_DIR*) (Thumb, 96 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = dir_remove(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> dir_next(FATFS_DIR*, int)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  - >> move_window(FATFS*, unsigned long)
  [Called By]
  - >> f_rename
  - >> f_unlink

  create_name(FATFS_DIR*, const char**) (Thumb, 534 bytes, Stack size 56 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = create_name(FATFS_DIR*, const char**) ⇒ mem_set(void*, int, unsigned)
  [Calls]
  - >> chk_chr(const char*, int)
  - >> mem_set(void*, int, unsigned)
  - >> ff_convert
  [Called By]
  - >> follow_path(FATFS_DIR*, const char*)

  get_fileinfo(FATFS_DIR*, FILINFO*) (Thumb, 296 bytes, Stack size 48 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = get_fileinfo(FATFS_DIR*, FILINFO*) ⇒ ff_convert
  [Calls]
  - >> ff_convert
  [Called By]
  - >> f_stat
  - >> f_readdir

  follow_path(FATFS_DIR*, const char*) (Thumb, 146 bytes, Stack size 32 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 248
  - Call Chain = follow_path(FATFS_DIR*, const char*) ⇒ dir_find(FATFS_DIR*) ⇒ dir_next(FATFS_DIR*, int) ⇒ create_chain(FATFS*, unsigned long) ⇒ put_fat(FATFS*, unsigned long, unsigned long) ⇒ move_window(FATFS*, unsigned long) ⇒ disk_write(unsigned char, const unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> create_name(FATFS_DIR*, const char**)
  - >> dir_find(FATFS_DIR*)
  - >> ld_clust(FATFS*, unsigned char*)
  - >> dir_sdi(FATFS_DIR*, unsigned short)
  [Called By]
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_stat
  - >> f_unlink
  - >> f_opendir
  - >> f_open
  - >> f_mkdir

  check_fs(FATFS*, unsigned long) (Thumb, 166 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = check_fs(FATFS*, unsigned long) ⇒ disk_read(unsigned char, unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  [Called By]
  - >> chk_mounted(const char**, FATFS**, unsigned char)

  chk_mounted(const char**, FATFS**, unsigned char) (Thumb, 904 bytes, Stack size 80 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = chk_mounted(const char**, FATFS**, unsigned char) ⇒ check_fs(FATFS*, unsigned long) ⇒ disk_read(unsigned char, unsigned char*, unsigned long, unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> check_fs(FATFS*, unsigned long)
  - >> disk_read(unsigned char, unsigned char*, unsigned long, unsigned char)
  - >> disk_status(unsigned char)
  - >> disk_initialize(unsigned char)
  [Called By]
  - >> f_rename
  - >> f_utime
  - >> f_chmod
  - >> f_getfree
  - >> f_stat
  - >> f_unlink
  - >> f_opendir
  - >> f_open
  - >> f_mkdir

  validate(void*) (Thumb, 52 bytes, Stack size 16 bytes, ff.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = validate(void*) ⇒ disk_status(unsigned char) ⇒ debug_if(int, const char*, ...) ⇒ __c89vfprintf
  [Calls]
  - >> disk_status(unsigned char)
  [Called By]
  - >> f_truncate
  - >> f_write
  - >> f_sync
  - >> f_read
  - >> f_lseek
  - >> f_readdir

  RTC_WriteAlarmCounter (Thumb, 132 bytes, Stack size 24 bytes, stm32f1xx_hal_rtc.o(i.RTC_WriteAlarmCounter))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC_WriteAlarmCounter
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_SetTime
  - >> HAL_RTC_SetDate
  - >> HAL_RTC_GetTime

  RTC_WriteTimeCounter (Thumb, 132 bytes, Stack size 24 bytes, stm32f1xx_hal_rtc.o(i.RTC_WriteTimeCounter))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC_WriteTimeCounter
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RTC_SetTime
  - >> HAL_RTC_SetDate
  - >> HAL_RTC_GetTime

  UART_SetConfig (Thumb, 284 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  gpio_irq0 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq0))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq0 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq1 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq1))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq1 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq2 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq2))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq2 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq3 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq3))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq3 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq4 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq4))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq4 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq5 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq5))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq5 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  gpio_irq6 (Thumb, 8 bytes, Stack size 0 bytes, gpio_irq_api.o(i.gpio_irq6))
  [Stack]

  - Max Depth = 32
  - Call Chain = gpio_irq6 ⇒ handle_interrupt_in
  [Calls]
  - >> handle_interrupt_in
  [Address Reference Count : 1]
  - gpio_irq_api.o(i.gpio_irq_init)

  handle_interrupt_in (Thumb, 114 bytes, Stack size 32 bytes, gpio_irq_api.o(i.handle_interrupt_in))
  [Stack]

  - Max Depth = 32
  - Call Chain = handle_interrupt_in
  [Called By]
  - >> gpio_irq6
  - >> gpio_irq5
  - >> gpio_irq4
  - >> gpio_irq3
  - >> gpio_irq2
  - >> gpio_irq1
  - >> gpio_irq0

  init_spi (Thumb, 72 bytes, Stack size 8 bytes, spi_api.o(i.init_spi))
  [Stack]

  - Max Depth = 16
  - Call Chain = init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> HAL_SPI_Init
  [Called By]
  - >> spi_init
  - >> spi_frequency
  - >> spi_format

  _fp_digits (Thumb, 326 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1762 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0vfprintf
  - >> __0sprintf
  - >> __0printf
  - >> __0fprintf

  _printf_post_padding (Thumb, 38 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 48 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  __default_terminate_handler() (Thumb, 6 bytes, Stack size 8 bytes, arm_exceptions_globs.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __default_terminate_handler()
  [Address Reference Count : 1]
  - arm_exceptions_globs.o(.text)

  ### Undefined Global Symbols