Static Call Graph - [.\build\Music Shield.axf]

# Static Call Graph for image .\build\Music Shield.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Mon Jul 27 18:43:00 2015

### Maximum Stack Usage = 264 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__sti___10_player_cpp ⇒ vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_IRQHandler ⇒ ADC1_IRQHandler

  ### Function Pointers

  - ADC1_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - BusFault_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - CAN_RX1_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - CAN_SCE_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - COMP2_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - COMP4_6_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - DebugMon_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI2_TSC_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - FLASH_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - FPU_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - HardFault_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - MemManage_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - NMI_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - PVD_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - PendSV_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - RCC_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - Reset_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - SPI2_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - SPI3_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - SVC_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - SysTick_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - SystemInit from system_stm32f3xx.o(i.SystemInit) referenced from startup_stm32f302x8.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM1_BRK_TIM15_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM1_TRG_COM_TIM17_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM1_UP_TIM16_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM2_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USART1_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USART2_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USART3_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USBWakeUp_RMP_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USB_HP_CAN_TX_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USB_HP_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USB_LP_CAN_RX0_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - USB_LP_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - UsageFault_Handler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - WWDG_IRQHandler from startup_stm32f302x8.o(.text) referenced from startup_stm32f302x8.o(RESET)
  - mbed::SPI::write(int) from SPI.o(i._ZN4mbed3SPI5writeEi) referenced from SPI.o(.constdata__ZTVN4mbed3SPIE)
  - vs10xx::~vs10xx() from player.o(i._ZN6vs10xxD1Ev) referenced from player.o(.text)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f302x8.o(.text)
  - __sti___10_player_cpp from player.o(.text) referenced from player.o(.init_array)
  - _sbackspace from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - _scanf_char_input from scanf_char.o(.text) referenced from scanf_char.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from __0sscanf.o(.text)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0fprintf)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0printf)
  - fputc from fputc_fp.o(.text) referenced from printfa.o(i.__0vfprintf)
  - isspace from isspace_c.o(.text) referenced from scanf_char.o(.text)
  - main from retarget.o(i.$Sub$$main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - timer_irq_handler from hal_tick.o(i.timer_irq_handler) referenced from hal_tick.o(i.HAL_InitTick)
  - us_ticker_clear_interrupt from us_ticker.o(i.us_ticker_clear_interrupt) referenced from us_ticker_api.o(.constdata)
  - us_ticker_disable_interrupt from us_ticker.o(i.us_ticker_disable_interrupt) referenced from us_ticker_api.o(.constdata)
  - us_ticker_init from us_ticker.o(i.us_ticker_init) referenced from us_ticker_api.o(.constdata)
  - us_ticker_read from us_ticker.o(i.us_ticker_read) referenced from us_ticker_api.o(.constdata)
  - us_ticker_set_interrupt from us_ticker.o(i.us_ticker_set_interrupt) referenced from us_ticker_api.o(.constdata)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  __use_full_stdio (Thumb, 0 bytes, Stack size unknown bytes, entry6b.o(.ARM.Collect$$$$00000006))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = __use_full_stdio ⇒ _initio ⇒ _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _initio

  __main_after_initio (Thumb, 0 bytes, Stack size unknown bytes, entry6b.o(.ARM.Collect$$$$00000006))
  [Called By]

  - >> _initio

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init$empty (Thumb, 0 bytes, Stack size unknown bytes, entry8a.o(.ARM.Collect$$$$00000009))
  [Stack]

  - Max Depth = 16 + Unknown Stack Size
  - Call Chain = _main_cpp_init$empty ⇒ __cpp_initialize__aeabi_
  [Calls]
  - >> __cpp_initialize__aeabi_

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  $Super$$main (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = $Super$$main ⇒ Player::beginMidi() ⇒ vs10xx::resetForMidi() ⇒ vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> Player::beginMidi()
  - >> Player::midiDemoPlayer()
  [Called By]
  - >> main

  Player::beginMidi() (Thumb, 24 bytes, Stack size 8 bytes, player.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = Player::beginMidi() ⇒ vs10xx::resetForMidi() ⇒ vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::resetForMidi()
  - >> __2printf
  [Called By]
  - >> $Super$$main

  Player::midiNoteOn(char, char, char) (Thumb, 30 bytes, Stack size 24 bytes, player.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = Player::midiNoteOn(char, char, char) ⇒ vs10xx::midiWriteData(char, char, char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::midiWriteData(char, char, char)
  [Called By]
  - >> Player::midiDemoPlayer()

  Player::midiNoteOff(char, char, char) (Thumb, 30 bytes, Stack size 24 bytes, player.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = Player::midiNoteOff(char, char, char) ⇒ vs10xx::midiWriteData(char, char, char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::midiWriteData(char, char, char)
  [Called By]
  - >> Player::midiDemoPlayer()

  Player::midiDemoPlayer() (Thumb, 134 bytes, Stack size 16 bytes, player.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = Player::midiDemoPlayer() ⇒ Player::midiNoteOff(char, char, char) ⇒ vs10xx::midiWriteData(char, char, char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> wait_ms
  - >> vs10xx::midiWriteData(char, char, char)
  - >> Player::midiNoteOff(char, char, char)
  - >> Player::midiNoteOn(char, char, char)
  - >> __2printf
  [Called By]
  - >> $Super$$main

  vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) (Thumb, 142 bytes, Stack size 40 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 240
  - Call Chain = vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::DigitalOut::DigitalOut(PinName)
  - >> gpio_init_in
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> __aeabi_memclr4
  [Called By]
  - >> __sti___10_player_cpp

  vs10xx::vs10xx__sub_object(PinName, PinName, PinName, PinName, PinName, PinName, PinName) (Thumb, 0 bytes, Stack size 40 bytes, vs10xx.o(.text), UNUSED)

  vs10xx::writeRegister(unsigned char, unsigned) (Thumb, 86 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::SPI::write(int)
  [Called By]
  - >> vs10xx::setVolume(unsigned char)
  - >> vs10xx::loadPlugin(const unsigned short*, int)
  - >> vs10xx::softReset()
  - >> vs10xx::resetForMidi()

  vs10xx::readRegister(unsigned char) (Thumb, 92 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed::DigitalIn::operator int()
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::SPI::write(int)
  [Called By]
  - >> vs10xx::softReset()

  vs10xx::writeData(unsigned char*, unsigned char) (Thumb, 76 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed::DigitalIn::operator int()
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::SPI::write(int)

  vs10xx::midiSendByte(char) (Thumb, 24 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = vs10xx::midiSendByte(char) ⇒ mbed::SPI::write(int) ⇒ spi_format ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> mbed::SPI::write(int)
  [Called By]
  - >> vs10xx::midiWriteData(char, char, char)

  vs10xx::midiWriteData(char, char, char) (Thumb, 100 bytes, Stack size 24 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = vs10xx::midiWriteData(char, char, char) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::DigitalOut::operator =(int)
  - >> vs10xx::midiSendByte(char)
  [Called By]
  - >> Player::midiNoteOff(char, char, char)
  - >> Player::midiNoteOn(char, char, char)
  - >> Player::midiDemoPlayer()

  vs10xx::softReset() (Thumb, 168 bytes, Stack size 8 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed::DigitalIn::operator int()
  - >> mbed::SPI::frequency(int)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> wait_ms
  - >> __2printf
  [Called By]
  - >> vs10xx::reset()

  vs10xx::reset() (Thumb, 66 bytes, Stack size 8 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::SPI::write(int)
  - >> vs10xx::softReset()
  - >> wait_ms

  vs10xx::loadPlugin(const unsigned short*, int) (Thumb, 116 bytes, Stack size 32 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  [Called By]
  - >> vs10xx::resetForMidi()

  vs10xx::resetForMidi() (Thumb, 128 bytes, Stack size 8 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = vs10xx::resetForMidi() ⇒ vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed::DigitalIn::operator int()
  - >> mbed::DigitalOut::operator =(int)
  - >> mbed::SPI::write(int)
  - >> vs10xx::loadPlugin(const unsigned short*, int)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> wait_ms
  [Called By]
  - >> Player::beginMidi()

  vs10xx::setFreq(int) (Thumb, 16 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> mbed::SPI::frequency(int)

  vs10xx::setVolume(unsigned char) (Thumb, 20 bytes, Stack size 16 bytes, vs10xx.o(.text), UNUSED)
  [Calls]

  - >> vs10xx::writeRegister(unsigned char, unsigned)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Calls]

  - >> ADC1_IRQHandler
  [Called By]
  - >> ADC1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  COMP2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  COMP4_6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI2_TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM1_BRK_TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM1_TRG_COM_TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM1_UP_TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USBWakeUp_RMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USB_HP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  USB_LP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f302x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f302x8.o(RESET)

  _initio (Thumb, 20 bytes, Stack size 0 bytes, initio_oe.o(.text))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = _initio ⇒ _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _sys_open
  - >> __main_after_initio
  [Called By]
  - >> __use_full_stdio

  fflush (Thumb, 38 bytes, Stack size 16 bytes, fflush_fe.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = fflush
  [Calls]
  - >> _sys_seek
  - >> _sys_ensure
  [Called By]
  - >> exit

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  ___aeabi_memcpy4$move (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  ___aeabi_memcpy8$move (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 64 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memmove (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memmove4 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memmove4
  [Called By]
  - >> NVIC_SetVector

  __aeabi_memmove8 (Thumb, 0 bytes, Stack size 8 bytes, memmovea.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> mbed::DigitalOut::DigitalOut(PinName)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> mbed::FileBase::lookup(const char*, unsigned)

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> _sys_open

  strncmp (Thumb, 30 bytes, Stack size 12 bytes, strncmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strncmp
  [Called By]
  - >> mbed::FileBase::lookup(const char*, unsigned)

  __0sscanf (Thumb, 48 bytes, Stack size 72 bytes, __0sscanf.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf_char
  [Called By]
  - >> _sys_open

  _scanf_int (Thumb, 336 bytes, Stack size 56 bytes, _scanf_int.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _scanf_int
  [Calls]
  - >> _chval
  [Called By]
  - >> __vfscanf

  __cpp_initialize__aeabi_ (Thumb, 22 bytes, Stack size 16 bytes, cpp_init.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __cpp_initialize__aeabi_
  [Called By]
  - >> _main_cpp_init$empty

  fputc (Thumb, 40 bytes, Stack size 16 bytes, fputc_fp.o(.text))
  [Stack]

  - Max Depth = 208
  - Call Chain = fputc ⇒ _sys_write ⇒ serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> _sys_write
  [Address Reference Count : 3]
  - printfa.o(i.__0fprintf)
  - printfa.o(i.__0printf)
  - printfa.o(i.__0vfprintf)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_int

  __vfscanf_char (Thumb, 20 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> __vfscanf
  [Called By]
  - >> __0sscanf

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - __0sscanf.o(.text)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  __rt_ddtor_pointer_addr (Thumb, 4 bytes, Stack size 0 bytes, cpp_dtor.o(.text))
  [Called By]

  - >> __aeabi_atexit
  - >> __cxa_finalize

  __rt_lib_shutdown_cpp_1 (Thumb, 2 bytes, Stack size 0 bytes, cpp_final.o(.text), UNUSED)

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text), UNUSED)
  [Calls]

  - >> _double_epilogue
  [Called By]
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 38 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  isspace (Thumb, 10 bytes, Stack size 0 bytes, isspace_c.o(.text))
  [Calls]

  - >> __ctype_lookup
  [Address Reference Count : 1]
  - scanf_char.o(.text)

  __vfscanf (Thumb, 806 bytes, Stack size 88 bytes, _scanf.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = __vfscanf ⇒ _scanf_int
  [Calls]
  - >> _scanf_int
  [Called By]
  - >> __vfscanf_char

  _double_round (Thumb, 26 bytes, Stack size 8 bytes, depilogue.o(.text), UNUSED)
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 164 bytes, Stack size 32 bytes, depilogue.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __ctype_lookup (Thumb, 34 bytes, Stack size 0 bytes, ctype_c.o(.text))
  [Called By]

  - >> isspace

  main (Thumb, 18 bytes, Stack size 8 bytes, retarget.o(i.$Sub$$main))
  [Stack]

  - Max Depth = 176
  - Call Chain = main ⇒ $Super$$main ⇒ Player::beginMidi() ⇒ vs10xx::resetForMidi() ⇒ vs10xx::loadPlugin(const unsigned short*, int) ⇒ vs10xx::writeRegister(unsigned char, unsigned) ⇒ mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_sdk_init
  - >> mbed_main
  - >> $Super$$main
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  HAL_GPIO_Init (Thumb, 502 bytes, Stack size 36 bytes, stm32f3xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> pin_function

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f3xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig
  - >> UART_WaitOnFlagUntilTimeout

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f3xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> timer_irq_handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f3xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_MspInit
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_InitTick
  [Called By]
  - >> SystemInit
  - >> mbed_sdk_init

  HAL_InitTick (Thumb, 128 bytes, Stack size 8 bytes, hal_tick.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_TIM_OC_Start
  - >> HAL_TIM_OC_Init
  - >> NVIC_SetVector
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init
  - >> us_ticker_read
  - >> us_ticker_init

  HAL_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal.o(i.HAL_MspInit))
  [Called By]

  - >> HAL_Init

  HAL_NVIC_SetPriorityGrouping (Thumb, 30 bytes, Stack size 0 bytes, stm32f3xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 730 bytes, Stack size 32 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_GetTick
  - >> HAL_InitTick
  [Called By]
  - >> SetSysClock

  HAL_RCC_GetPCLK1Freq (Thumb, 64 bytes, Stack size 8 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 64 bytes, Stack size 8 bytes, stm32f3xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 98 bytes, Stack size 0 bytes, stm32f3xx_hal_rcc_ex.o(i.HAL_RCC_GetSysClockFreq))
  [Called By]

  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  - >> UART_SetConfig

  HAL_RCC_OscConfig (Thumb, 1414 bytes, Stack size 40 bytes, stm32f3xx_hal_rcc_ex.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SetSysClock

  HAL_SPI_Init (Thumb, 224 bytes, Stack size 16 bytes, stm32f3xx_hal_spi.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> init_spi

  HAL_SPI_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal_spi.o(i.HAL_SPI_MspInit))
  [Called By]

  - >> HAL_SPI_Init

  HAL_TIM_OC_Init (Thumb, 50 bytes, Stack size 8 bytes, stm32f3xx_hal_tim.o(i.HAL_TIM_OC_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_TIM_OC_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_OC_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> HAL_InitTick

  HAL_TIM_OC_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal_tim.o(i.HAL_TIM_OC_MspInit))
  [Called By]

  - >> HAL_TIM_OC_Init

  HAL_TIM_OC_Start (Thumb, 84 bytes, Stack size 0 bytes, stm32f3xx_hal_tim.o(i.HAL_TIM_OC_Start))
  [Called By]

  - >> HAL_InitTick

  HAL_UART_Init (Thumb, 106 bytes, Stack size 8 bytes, stm32f3xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Init ⇒ UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> serial_init

  HAL_UART_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f3xx_hal_uart.o(i.HAL_UART_MspInit))
  [Called By]

  - >> HAL_UART_Init

  NVIC_SetVector (Thumb, 98 bytes, Stack size 24 bytes, cmsis_nvic.o(i.NVIC_SetVector))
  [Stack]

  - Max Depth = 32
  - Call Chain = NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> __aeabi_memmove4
  [Called By]
  - >> HAL_InitTick

  SetSysClock (Thumb, 188 bytes, Stack size 96 bytes, system_stm32f3xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 168
  - Call Chain = SetSysClock ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCC_OscConfig
  [Called By]
  - >> SystemInit

  Set_GPIO_Clock (Thumb, 86 bytes, Stack size 8 bytes, pinmap.o(i.Set_GPIO_Clock))
  [Stack]

  - Max Depth = 96
  - Call Chain = Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> gpio_init
  - >> pin_mode
  - >> pin_function

  SystemCoreClockUpdate (Thumb, 96 bytes, Stack size 4 bytes, system_stm32f3xx.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 4
  - Call Chain = SystemCoreClockUpdate
  [Called By]
  - >> mbed_sdk_init

  SystemInit (Thumb, 116 bytes, Stack size 8 bytes, system_stm32f3xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 176
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SetSysClock
  - >> HAL_Init
  [Address Reference Count : 1]
  - startup_stm32f302x8.o(.text)

  TIM_Base_SetConfig (Thumb, 102 bytes, Stack size 12 bytes, stm32f3xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_OC_Init

  UART_AdvFeatureConfig (Thumb, 218 bytes, Stack size 0 bytes, stm32f3xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Called By]

  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 84 bytes, Stack size 16 bytes, stm32f3xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 428 bytes, Stack size 16 bytes, stm32f3xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 162 bytes, Stack size 32 bytes, stm32f3xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> UART_CheckIdleState

  mbed::DigitalOut::DigitalOut(PinName) (Thumb, 26 bytes, Stack size 16 bytes, vs10xx.o(i._ZN4mbed10DigitalOutC1E7PinName))
  [Stack]

  - Max Depth = 184
  - Call Chain = mbed::DigitalOut::DigitalOut(PinName) ⇒ gpio_init_out ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_init_out
  - >> __aeabi_memclr4
  [Called By]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  mbed::DigitalOut::DigitalOut__sub_object(PinName) (Thumb, 0 bytes, Stack size 16 bytes, vs10xx.o(i._ZN4mbed10DigitalOutC1E7PinName), UNUSED)

  mbed::DigitalOut::operator =(int) (Thumb, 22 bytes, Stack size 16 bytes, vs10xx.o(i._ZN4mbed10DigitalOutaSEi))
  [Stack]

  - Max Depth = 104
  - Call Chain = mbed::DigitalOut::operator =(int) ⇒ gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_write(gpio_t*, int)
  [Called By]
  - >> vs10xx::reset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> vs10xx::midiWriteData(char, char, char)
  - >> vs10xx::resetForMidi()

  mbed::SPI::write(int) (Thumb, 48 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPI5writeEi))
  [Stack]

  - Max Depth = 48
  - Call Chain = mbed::SPI::write(int) ⇒ spi_format ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> spi_master_write
  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> vs10xx::reset()
  - >> vs10xx::midiSendByte(char)
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> vs10xx::resetForMidi()
  [Address Reference Count : 1]
  - SPI.o(.constdata__ZTVN4mbed3SPIE)

  mbed::SPI::frequency(int) (Thumb, 36 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPI9frequencyEi), UNUSED)
  [Calls]

  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> vs10xx::setFreq(int)
  - >> vs10xx::softReset()

  mbed::SPI::SPI(PinName, PinName, PinName, PinName) (Thumb, 74 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPIC1E7PinNameS1_S1_S1_))
  [Stack]

  - Max Depth = 200
  - Call Chain = mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> spi_init
  - >> spi_frequency
  - >> spi_format
  [Called By]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  mbed::SPI::SPI__sub_object(PinName, PinName, PinName, PinName) (Thumb, 0 bytes, Stack size 16 bytes, SPI.o(i._ZN4mbed3SPIC1E7PinNameS1_S1_S1_), UNUSED)

  mbed::FileBase::getPathType() (Thumb, 4 bytes, Stack size 0 bytes, FileBase.o(i._ZN4mbed8FileBase11getPathTypeEv))
  [Called By]

  - >> mbed::FilePath::isFile()
  - >> mbed::FilePath::file()
  - >> mbed::FilePath::fileSystem()

  mbed::FileBase::lookup(const char*, unsigned) (Thumb, 50 bytes, Stack size 16 bytes, FileBase.o(i._ZN4mbed8FileBase6lookupEPKcj))
  [Stack]

  - Max Depth = 28
  - Call Chain = mbed::FileBase::lookup(const char*, unsigned) ⇒ strncmp
  [Calls]
  - >> strncmp
  - >> strlen
  [Called By]
  - >> mbed::FilePath::FilePath(const char*)

  mbed::FilePath::fileSystem() (Thumb, 24 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath10fileSystemEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::fileSystem()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> _sys_open

  mbed::FilePath::file() (Thumb, 28 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath4fileEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::file()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> _sys_open

  mbed::FilePath::exists() (Thumb, 10 bytes, Stack size 0 bytes, FilePath.o(i._ZN4mbed8FilePath6existsEv))
  [Called By]

  - >> _sys_open

  mbed::FilePath::isFile() (Thumb, 24 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePath6isFileEv))
  [Stack]

  - Max Depth = 8
  - Call Chain = mbed::FilePath::isFile()
  [Calls]
  - >> mbed::FileBase::getPathType()
  [Called By]
  - >> _sys_open

  mbed::FilePath::fileName() (Thumb, 4 bytes, Stack size 0 bytes, FilePath.o(i._ZN4mbed8FilePath8fileNameEv))
  [Called By]

  - >> _sys_open

  mbed::FilePath::FilePath(const char*) (Thumb, 64 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePathC1EPKc))
  [Stack]

  - Max Depth = 36
  - Call Chain = mbed::FilePath::FilePath(const char*) ⇒ mbed::FileBase::lookup(const char*, unsigned) ⇒ strncmp
  [Calls]
  - >> mbed::FileBase::lookup(const char*, unsigned)
  [Called By]
  - >> _sys_open

  mbed::FilePath::FilePath__sub_object(const char*) (Thumb, 0 bytes, Stack size 8 bytes, FilePath.o(i._ZN4mbed8FilePathC1EPKc), UNUSED)

  mbed::DigitalIn::operator int() (Thumb, 52 bytes, Stack size 8 bytes, vs10xx.o(i._ZN4mbed9DigitalIncviEv))
  [Stack]

  - Max Depth = 80
  - Call Chain = mbed::DigitalIn::operator int() ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  [Called By]
  - >> vs10xx::softReset()
  - >> vs10xx::writeData(unsigned char*, unsigned char)
  - >> vs10xx::readRegister(unsigned char)
  - >> vs10xx::writeRegister(unsigned char, unsigned)
  - >> vs10xx::midiWriteData(char, char, char)
  - >> vs10xx::resetForMidi()

  vs10xx::~vs10xx() (Thumb, 4 bytes, Stack size 0 bytes, player.o(i._ZN6vs10xxD1Ev))
  [Address Reference Count : 1]

  - player.o(.text)

  vs10xx::~vs10xx__sub_object() (Thumb, 0 bytes, Stack size 0 bytes, player.o(i._ZN6vs10xxD1Ev), UNUSED)

  __0fprintf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)
  [Calls]

  - >> _printf_core

  __1fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  __2fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2fprintf
  [Called By]
  - >> mbed_assert_internal

  __c89fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  fprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0fprintf), UNUSED)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> vs10xx::softReset()
  - >> Player::beginMidi()
  - >> Player::midiDemoPlayer()

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __0vfprintf (Thumb, 20 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)
  [Calls]

  - >> _printf_core

  __1vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)

  __2vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)

  __c89vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf), UNUSED)

  vfprintf (Thumb, 0 bytes, Stack size 8 bytes, printfa.o(i.__0vfprintf))
  [Stack]

  - Max Depth = 8
  - Call Chain = vfprintf
  [Called By]
  - >> error

  __aeabi_atexit (Thumb, 50 bytes, Stack size 24 bytes, aeabi_atexit.o(i.__aeabi_atexit))
  [Stack]

  - Max Depth = 44
  - Call Chain = __aeabi_atexit ⇒ malloc
  [Calls]
  - >> __rt_ddtor_pointer_addr
  - >> malloc
  [Called By]
  - >> __sti___10_player_cpp

  __cxa_finalize (Thumb, 66 bytes, Stack size 24 bytes, cxa_finalize.o(i.__cxa_finalize), UNUSED)
  [Calls]

  - >> __rt_ddtor_pointer_addr
  - >> free

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  _sys_ensure (Thumb, 34 bytes, Stack size 0 bytes, retarget.o(i._sys_ensure))
  [Called By]

  - >> fflush

  _sys_open (Thumb, 212 bytes, Stack size 32 bytes, retarget.o(i._sys_open))
  [Stack]

  - Max Depth = 248
  - Call Chain = _sys_open ⇒ __0sscanf ⇒ __vfscanf_char ⇒ __vfscanf ⇒ _scanf_int
  [Calls]
  - >> mbed::FilePath::FilePath(const char*)
  - >> mbed::FilePath::fileName()
  - >> mbed::FilePath::isFile()
  - >> mbed::FilePath::exists()
  - >> mbed::FilePath::file()
  - >> mbed::FilePath::fileSystem()
  - >> strcmp
  - >> __0sscanf
  [Called By]
  - >> _initio

  _sys_seek (Thumb, 36 bytes, Stack size 0 bytes, retarget.o(i._sys_seek))
  [Called By]

  - >> fflush

  _sys_write (Thumb, 82 bytes, Stack size 16 bytes, retarget.o(i._sys_write))
  [Stack]

  - Max Depth = 192
  - Call Chain = _sys_write ⇒ serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> serial_putc
  - >> serial_init
  [Called By]
  - >> fputc

  error (Thumb, 20 bytes, Stack size 24 bytes, error.o(i.error))
  [Stack]

  - Max Depth = 88
  - Call Chain = error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> exit
  - >> vfprintf
  [Called By]
  - >> Set_GPIO_Clock
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge

  exit (Thumb, 24 bytes, Stack size 0 bytes, retarget.o(i.exit))
  [Stack]

  - Max Depth = 64
  - Call Chain = exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_die
  - >> fflush
  [Called By]
  - >> error

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free), UNUSED)
  [Called By]

  - >> __cxa_finalize

  gpio_dir (Thumb, 52 bytes, Stack size 16 bytes, gpio_api.o(i.gpio_dir))
  [Stack]

  - Max Depth = 152
  - Call Chain = gpio_dir ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> pin_function
  [Called By]
  - >> gpio_init_out
  - >> gpio_init_in

  gpio_init (Thumb, 60 bytes, Stack size 16 bytes, gpio_api.o(i.gpio_init))
  [Stack]

  - Max Depth = 152
  - Call Chain = gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> Set_GPIO_Clock
  - >> pin_function
  [Called By]
  - >> gpio_init_out
  - >> gpio_init_in

  gpio_init_in (Thumb, 38 bytes, Stack size 16 bytes, gpio.o(i.gpio_init_in))
  [Stack]

  - Max Depth = 168
  - Call Chain = gpio_init_in ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> gpio_mode
  - >> gpio_init
  - >> gpio_dir
  [Called By]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)

  gpio_init_out (Thumb, 64 bytes, Stack size 16 bytes, gpio.o(i.gpio_init_out))
  [Stack]

  - Max Depth = 168
  - Call Chain = gpio_init_out ⇒ gpio_init ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> gpio_mode
  - >> gpio_init
  - >> gpio_dir
  [Called By]
  - >> mbed::DigitalOut::DigitalOut(PinName)

  gpio_mode (Thumb, 8 bytes, Stack size 0 bytes, gpio_api.o(i.gpio_mode))
  [Stack]

  - Max Depth = 112
  - Call Chain = gpio_mode ⇒ pin_mode ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> pin_mode
  [Called By]
  - >> gpio_init_out
  - >> gpio_init_in

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> __aeabi_atexit

  mbed_assert_internal (Thumb, 24 bytes, Stack size 8 bytes, assert.o(i.mbed_assert_internal))
  [Stack]

  - Max Depth = 72
  - Call Chain = mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_die
  - >> __2fprintf
  [Called By]
  - >> mbed::DigitalIn::operator int()
  - >> gpio_init_out
  - >> gpio_write(gpio_t*, int)
  - >> serial_init
  - >> gpio_dir
  - >> spi_init
  - >> pin_mode
  - >> pin_function

  mbed_die (Thumb, 16 bytes, Stack size 0 bytes, board.o(i.mbed_die))
  [Stack]

  - Max Depth = 64
  - Call Chain = mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> wait_ms
  [Called By]
  - >> mbed_assert_internal
  - >> exit

  mbed_main (Thumb, 2 bytes, Stack size 0 bytes, retarget.o(i.mbed_main))
  [Called By]

  - >> main

  mbed_sdk_init (Thumb, 14 bytes, Stack size 8 bytes, mbed_overrides.o(i.mbed_sdk_init))
  [Stack]

  - Max Depth = 56
  - Call Chain = mbed_sdk_init ⇒ HAL_Init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> SystemCoreClockUpdate
  - >> HAL_Init
  [Called By]
  - >> main

  pin_function (Thumb, 78 bytes, Stack size 40 bytes, pinmap.o(i.pin_function))
  [Stack]

  - Max Depth = 136
  - Call Chain = pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> HAL_GPIO_Init
  - >> Set_GPIO_Clock
  [Called By]
  - >> gpio_init
  - >> gpio_dir
  - >> pinmap_pinout

  pin_mode (Thumb, 62 bytes, Stack size 16 bytes, pinmap.o(i.pin_mode))
  [Stack]

  - Max Depth = 112
  - Call Chain = pin_mode ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> Set_GPIO_Clock
  [Called By]
  - >> serial_init
  - >> gpio_mode
  - >> pinmap_pinout

  pinmap_merge (Thumb, 34 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_merge))
  [Stack]

  - Max Depth = 96
  - Call Chain = pinmap_merge ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> serial_init
  - >> spi_init

  pinmap_peripheral (Thumb, 58 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_peripheral))
  [Stack]

  - Max Depth = 96
  - Call Chain = pinmap_peripheral ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  [Called By]
  - >> serial_init
  - >> spi_init

  pinmap_pinout (Thumb, 66 bytes, Stack size 8 bytes, pinmap_common.o(i.pinmap_pinout))
  [Stack]

  - Max Depth = 144
  - Call Chain = pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> error
  - >> pin_mode
  - >> pin_function
  [Called By]
  - >> serial_init
  - >> spi_init

  serial_init (Thumb, 340 bytes, Stack size 32 bytes, serial_api.o(i.serial_init))
  [Stack]

  - Max Depth = 176
  - Call Chain = serial_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> HAL_UART_Init
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge
  - >> pin_mode
  [Called By]
  - >> _sys_write

  serial_putc (Thumb, 38 bytes, Stack size 0 bytes, serial_api.o(i.serial_putc))
  [Called By]

  - >> _sys_write

  spi_format (Thumb, 96 bytes, Stack size 8 bytes, spi_api.o(i.spi_format))
  [Stack]

  - Max Depth = 32
  - Call Chain = spi_format ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> init_spi
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::SPI::frequency(int)
  - >> mbed::SPI::write(int)

  spi_frequency (Thumb, 120 bytes, Stack size 0 bytes, spi_api.o(i.spi_frequency))
  [Stack]

  - Max Depth = 24
  - Call Chain = spi_frequency ⇒ init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> init_spi
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)
  - >> mbed::SPI::frequency(int)
  - >> mbed::SPI::write(int)

  spi_init (Thumb, 218 bytes, Stack size 40 bytes, spi_api.o(i.spi_init))
  [Stack]

  - Max Depth = 184
  - Call Chain = spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  - >> init_spi
  - >> pinmap_pinout
  - >> pinmap_peripheral
  - >> pinmap_merge
  [Called By]
  - >> mbed::SPI::SPI(PinName, PinName, PinName, PinName)

  spi_master_write (Thumb, 70 bytes, Stack size 0 bytes, spi_api.o(i.spi_master_write))
  [Called By]

  - >> mbed::SPI::write(int)

  ticker_irq_handler (Thumb, 78 bytes, Stack size 8 bytes, ticker_api.o(i.ticker_irq_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ticker_irq_handler
  [Called By]
  - >> us_ticker_irq_handler

  timer_irq_handler (Thumb, 76 bytes, Stack size 16 bytes, hal_tick.o(i.timer_irq_handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = timer_irq_handler ⇒ us_ticker_irq_handler ⇒ ticker_irq_handler
  [Calls]
  - >> HAL_IncTick
  - >> us_ticker_irq_handler
  [Address Reference Count : 1]
  - hal_tick.o(i.HAL_InitTick)

  us_ticker_clear_interrupt (Thumb, 12 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_clear_interrupt))
  [Address Reference Count : 1]

  - us_ticker_api.o(.constdata)

  us_ticker_disable_interrupt (Thumb, 14 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_disable_interrupt))
  [Address Reference Count : 1]

  - us_ticker_api.o(.constdata)

  us_ticker_init (Thumb, 26 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_init))
  [Stack]

  - Max Depth = 40
  - Call Chain = us_ticker_init ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_InitTick
  [Address Reference Count : 1]
  - us_ticker_api.o(.constdata)

  us_ticker_irq_handler (Thumb, 6 bytes, Stack size 0 bytes, us_ticker_api.o(i.us_ticker_irq_handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = us_ticker_irq_handler ⇒ ticker_irq_handler
  [Calls]
  - >> ticker_irq_handler
  [Called By]
  - >> timer_irq_handler

  us_ticker_read (Thumb, 30 bytes, Stack size 8 bytes, us_ticker.o(i.us_ticker_read))
  [Stack]

  - Max Depth = 48
  - Call Chain = us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> HAL_InitTick
  [Called By]
  - >> wait_ms
  [Address Reference Count : 1]
  - us_ticker_api.o(.constdata)

  us_ticker_set_interrupt (Thumb, 16 bytes, Stack size 0 bytes, us_ticker.o(i.us_ticker_set_interrupt))
  [Address Reference Count : 1]

  - us_ticker_api.o(.constdata)

  wait_ms (Thumb, 28 bytes, Stack size 16 bytes, wait_api.o(i.wait_ms))
  [Stack]

  - Max Depth = 64
  - Call Chain = wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> us_ticker_read
  [Called By]
  - >> vs10xx::reset()
  - >> vs10xx::softReset()
  - >> vs10xx::resetForMidi()
  - >> Player::midiDemoPlayer()
  - >> mbed_die

  ### Local Symbols

  __sti___10_player_cpp (Thumb, 42 bytes, Stack size 24 bytes, player.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = __sti___10_player_cpp ⇒ vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName) ⇒ mbed::SPI::SPI(PinName, PinName, PinName, PinName) ⇒ spi_init ⇒ pinmap_pinout ⇒ pin_function ⇒ Set_GPIO_Clock ⇒ error ⇒ exit ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> vs10xx::vs10xx(PinName, PinName, PinName, PinName, PinName, PinName, PinName)
  - >> __aeabi_atexit
  [Address Reference Count : 1]
  - player.o(.init_array)

  gpio_write(gpio_t*, int) (Thumb, 46 bytes, Stack size 16 bytes, vs10xx.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = gpio_write(gpio_t*, int) ⇒ mbed_assert_internal ⇒ mbed_die ⇒ wait_ms ⇒ us_ticker_read ⇒ HAL_InitTick ⇒ NVIC_SetVector ⇒ __aeabi_memmove4
  [Calls]
  - >> mbed_assert_internal
  [Called By]
  - >> mbed::DigitalOut::operator =(int)

  init_spi (Thumb, 72 bytes, Stack size 8 bytes, spi_api.o(i.init_spi))
  [Stack]

  - Max Depth = 24
  - Call Chain = init_spi ⇒ HAL_SPI_Init
  [Calls]
  - >> HAL_SPI_Init
  [Called By]
  - >> spi_init
  - >> spi_frequency
  - >> spi_format

  _fp_digits (Thumb, 326 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1762 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0vfprintf
  - >> __0printf
  - >> __0fprintf

  _printf_post_padding (Thumb, 38 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 48 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _scanf_char_input (Thumb, 12 bytes, Stack size 0 bytes, scanf_char.o(.text))
  [Address Reference Count : 1]

  - scanf_char.o(.text)

  ### Undefined Global Symbols